# Performing Runtime Shutdown and Reboot

- Shutdown
- Reboot

## Shutdown

The following occurs when you perform shutdown.

- If script is set up with the [Stop] runtime application trigger, the specified operation is run.
- Communication with external devices is stopped.
- The runtime application ends.
- When using models other than SP5000 Series Open Box (Windows 10 IoT Enterprise Model), IPC series, or PC/AT, the display unit is shutdown.

Note: When using models other than SP5000 Series Open Box (Windows 10 IoT Enterprise Model), IPC series, or PC/AT, to power up after the display unit is shutdown, disconnect the power cable and reconnect again.

To shutdown runtime, do one of the following:

- Open the Hardware Configuration screen and touch the [Shutdown] button.

- Run the script (runtime application's [Shutdown] operation).
  (Example)

- For SP5000 Series Open Box (Windows 10 IoT Enterprise Model), IPC Series, and PC/AT, click the [x] at the top right of the runtime application.

## Reboot

The following occurs when you perform reboot.

- If script is set up with the [Stop] runtime application trigger, the specified operation is run.
- Communication with external devices is stopped.
- The runtime application ends, and is restarted.

To restart runtime, do one of the following:

- Open the Hardware Configuration screen and touch the [Reboot] button.

- Run the script (runtime application's [Reboot] operation).

(Example)