# Variables

Property | Description | Data Type | Minimum Value | Maximum Value | Read | Write
InitialValue | Stores the initial value for the internal variable. | BOOL, Integer, Real, Date, Time, Date And Time, String | Default value of the selected data type. | Default value of the selected data type. |  | -
Min | Stores the minimum value for data input to the variable. | BOOL, Integer, Real, Date, Time, Date And Time, String | Default value of the selected data type. | Default value of the selected data type. |  | -
Max | Stores the maximum value for data input to the variable. | BOOL, Integer, Real, Date, Time, Date And Time, String | Default value of the selected data type. | Default value of the selected data type. |  | -
Value | Stores the variable value. | BOOL, Integer, Real, Date, Time, Date And Time, String | Default value of the selected data type. | Default value of the selected data type. |  |
Quality Note: This property is not available for local variables. | Displays the scan status of the selected variable.
Value | Description
0, 4 | Access to device address and device address value is normal.
1, 3, 5, 7 | Cannot access the device address.
6 | After the display unit starts and accesses the device address, the display unit is in a waiting state, until the device address value becomes available.
8, 12 | Device address value is invalid.
9, 13, 15 | You cannot access the device address. Also, the device address value can be invalid.
2, 10, 11, 14 | Not in use
| BYTE | 0 | 15 |  | -