# Configuring EcoStruxure Augmented Operator Advisor

This section describes the steps to configure the EcoStruxure Augmented Operator Advisor Settings.

Note:

- For information on the models which support the EcoStruxure Augmented Operator Advisor, see the following.

  Supported Model/Feature.

- For more details on EcoStruxure Augmented Operator Advisor Configuration, refer following manuals.

  Manual | Link
  EcoStruxure Augmented Operator Advisor Quick Start Guide | EN, FR, DE, ES, IT, CN
  EcoStruxure Augmented Operator Advisor Manager User Manual | EN, FR, DE, ES, IT, CN
  EcoStruxure Augmented Operator Advisor App User Manual | EN, FR, DE, ES, IT, CN
  EcoStruxure Augmented Operator Advisor Builder User Manual | EN, FR, DE, ES, IT, CN

  DE(German), EN(English), FR(French), IT(Italian), ES(Spanish), CN(Chinese)

1. In Project Explorer window, go to [System Architecture] and click [Driver].

2. On Project Explorer window toolbar, click [Driver].
   → An Add Driver window opens.

3. From the [Manufacturer] list select [Schneider Electric], then from [Driver] select [EcoStruxure Augmented Operator Advisor] and click [OK].

4. In Properties window, go to [Basic] tab and configure the [Timeout(sec)] setting of the driver.

5. On the System Architecture document view, click the equipment. (EcoStruxureAugmentedOperatorAdvisorEquipment1)

6. In Properties window, go to [Basic] tab and configure the port number and IP address of the equipment.