APP10101

Other Recipe operation is executing.

Carrying out the different Recipe Group operation.

Carry out the operation after precedent processing is finished, or change the operation order.

APP10110

Recipe Create operation failed.

Exceeds the maximum number of recipes that one recipe group can set, or corresponding recipe group ID does not exist.

Set the number of recipes to 256 or less and confirm the correct ID in Recipe Listbox.

APP10120

Recipe Delete operation failed.

Corresponding data ID does not exist.

Confirm the correct ID in Recipe Listbox.

APP10130

Recipe Save operation failed.

APP10140

Recipe Load operation failed.

APP10150

Recipe Send operation failed.

-

Verify the following and try again.
1. Confirm the corresponding data ID in Recipe Listbox.
2. Confirm if the specified external device is correct, and check the connection state of the communication cable.

APP10160

Recipe Snapshot operation failed.

APP10170

Recipe Compare operation failed.

Verify the following and try again.
1. Confirm the corresponding data ID in Recipe Listbox.
2. Confirm if the specified external device is correct, and check the connection state of the communication cable.
3. Compare the data with screen editing software and confirm if unnecessary variable is not added by the data import.

APP10180

Recipe Import operation failed.

Verify the following and try again.
1. Confirm the corresponding data ID in Recipe Listbox.
2. Confirm the imported file exists in external storage, and that the file format has not changed.
3. Confirm '+', '-', '=', '@', [TAB], and [ENTER] characters are not being used in item names.
4. Confirm the number of characters has not exceeded the maximum limit.

APP10181

Unable to import file because it was created using an incompatible version.

File was created using an incompatible version of the screen editing software.

Import a file exported from either the same version, or a compatible version, of the screen editing software.

APP10190

Recipe Export operation failed.

Verify the following and try again.
1. Confirm the corresponding data ID in Recipe Listbox.
2. Confirm if the file is not read-only and check the connection state / space of external storage.

APP10201

%s: Invalid value for equipment property.

Tried to set a value that is not supported by 'OverwriteValue' of the equipment property.

Set a supported value in 'OverwriteValue' of the equipment property.

APP10507

File open error. Application cannot open the file.

Backup file to restore does not exist.

Carry out the restore in a state with the backup file.

APP10509

Composition error.

The system structure of external device is different from creating the backup file.

Unify the combinations of system structure (CPU, Link I/F, communication method) with the backup file.

APP10511

The equipment is not connected.

Display unit and external device is not communicating.

Turn OFF the display unit and confirm the wiring of cables and connectors.

APP10512

System configuration is different.

Model of external device is different from creating the backup file. Unify it.

APP10513

Backup/Restore failed. 2 or more ChainData of Azbil is not supported.

Multiple chain backup and restore is not supported.

Carry out in single chain structure.

APP10601

External storage is not inserted.

External storage is required to export the operation log data.

Insert external storage.

APP10602

External storage does not have enough free space.

External storage needs 1 MB or more free space to export the operation log data.

Check whether the external storage has sufficient space.

APP10603

Failed to export the operation log data to the external storage.

External storage is removed or not inserted properly.
SD Card is write protected.

Check whether the external storage is inserted properly.
Release the lock of SD Card.

APP10604

Number of files in the export folder have exceeded the limit.

When the operation log data is exported to the external storage, number of files in the export folder have exceeded the limit (maximum 1000 files).

Change the external storage.
Remove the files from the export folder.

APP10701

Failed to copy/paste files.

1.Check whether the external storage has sufficient space.
2.Check whether the external storage is inserted properly.
3.When using a model that can set write filter (write protection), remove the setting.
4.Confirm if the file is not read-only.
5.When using File Management operation, confirm the settings.

APP10702

Failed to cut/paste files.

APP10703

Failed to delete files.

APP10801

%s: TCP port number (%d) is used by multiple functions.
(%s = "Web Viewer / WebServer", %d = Port number)

TCP port number on the display unit is used by multiple functions.

Change the port number of either the Web function or PLC driver.
Configuring the Server

APP10901

Unable to load content (ID %d) in [%s] on screen (ID %d). The total number of local variables on the screen and content has reached its limit.

The total number of local variables on the screen and content has reached its limit.

Reduce the number of local variables used on the content or screen.

APP10902

Unable to load screen: ID %d. The number of local variables on the screen has reached its limit.

The number of local variables on the screen has reached its limit.

Reduce the number of local variables used on the screen.

APP10903

Unable to load content (ID: %d, %s) onto screen (ID: %d).
The number of objects on the screen and content has reached the limit.

The count for objects on the screen and content has reached the limit.

Reduce the number of objects on the content or screen.

APP10904

Unable to load screen: ID %d. The number of objects on the screen has reached its limit.

The count for objects on the screen has reached its limit.

Reduce the number of objects on the screen.

APP11001

Failed to connect to FTP server (%s).

The configured FTP server address is incorrect. For example, the FTP server may not be connected to the network.

Check the FTP server address. Check the status of the network.

APP11002

Login to the FTP server (%s) failed.

The configured user name and password are incorrect.

Check the user name and password.

APP11003

FTP connection ID is unavailable.

The FTP connection ID is outside the range or the server information of the FTP connection ID may not be registered.

Check the FTP Connection ID.

APP11004

SSL/TLS communication with FTP server (%s) failed.

TLS communication failed.

1. Confirm that the FTP server supports FTPS.
2. Confirm that the TLS version of the FTP server is compatible with the version of the display unit.
3. Confirm that the FTP server's encryption suite is compatible with the display unit's version.
4. Confirm SSL/TLS is not blocked in the communication path.

APP11005

SSL/TLS connection with FTP server (%s) failed. The root certificate is invalid.

The root certificate file is invalid.

Check the contents of the root certificate file and re-transfer the project.

APP11006

SSL/TLS connection with FTP server (%s) failed due to server certificate validation error.

Server certificate validation error.

1. Ensure the server certificate is within its validity period.
2. Verify the system date and time on the display unit are correct.
3. Check if the certificate on the FTP server is correct.

APP11021

Failed to download file (%s) from FTP server (%s).

The specified file path is incorrect. The file does not exist on the FTP server.

Check the file path. Check the file on the FTP server.

APP11022

Failed to download file (%s) due to communication error with FTP server (%s).

The network is disconnected. For example, the FTP server may be down.

Check the status of the network and FTP server.

APP11023

Failed to download from FTP server (%s) due to write error in file (%s).

Failed to write to file.

1. Check that there is sufficient capacity in the write destination.
2. Check that the file path to write to is correct.
3. Check that the destination is not write-protected.

APP11031

Failed to upload file (%s) to FTP server (%s).

The specified file path is incorrect. The file cannot be written to the FTP server.

Check the file path. Check if the file is writeable on the FTP server.

APP11032

Failed to upload file (%s) due to communication error with FTP server (%s).

APP11033

Failed to upload to FTP server (%s) due to a read file error (%s).

Failed to load the file.

1. Check that the file you are loading exists.
2. Check that the path of the file to load is correct.

APP11041

FTP connection interrupted due to exceeding limitations.

The connection was interrupted because it exceeded the file limitations.
The number of files exceeded 1000 in the FTP connection.

In the Remote File Management, check the number of target files.

APP11091

Unexpected error (Internal Error No.:%s) occurred while connecting to FTP server (%s).

Unexpected error during FTP communication.

Check if the FTP server address is correct. Check the status of the network.

SYS00001

Target is write protected.

System of the display unit is write protected.

1. Release the lock switch of the SD card.
2. When using a model that can set write filter (write protection), remove the setting.

SYS00002

Invalid path (%s).

Unable to access the project file stored in external storage.

Confirm an abnormality in external storage and download the data which you uploaded to external storage again to the display unit.

SYS00003

The backup file is corrupted.

Backup file got corrupted during downloading the project file to display unit.

SYS00006

Display unit model differs between the model selected in project file and the one you are using.

Change the display unit model in project file to the one you are using.

SYS00008

The system version (%s) is lower than current system version (%s), during the %s process.

The project on the external storage has a lower run-time version than the display unit.

You can use either of the solution:
1. Downgrade run-time version on the display unit by downloading project file through ethernet or USB cable.
2. Download the project file developed in the editor having the same run-time version.

SYS00010

Not enough space (%s) on this product, during the %s process. Minimum space required is %s.

The data size of the project file exceeds the display unit's free space.

Decrease the data size.

SYS00011

Restore of %s from the backup file failed during the %s process.

Data could not be written during downloading the project file to display unit via external storage.

Restart the display unit and download the data again.

SYS00012

Extraction of %s archive failed during the %s process.

Data could not be written during downloading the project file to display unit.

SYS00014

The upload type (%s) is not supported in this version.

Unable to transfer because the system (Runtime) of the target is out of date.

Download the project file to the display unit again. Runtime is updated.

SYS00015

%s archive creation failed during the %s process.

External Storage / hard disk do not have enough free space or unable to access.

Confirm whether the disk space is sufficient, not read-only and has access privileges.

SYS00016

Response not received during the %s process.

USB transfer cable is not properly recognized or communication is blocked by a firewall.

1. When using USB transfer cable, confirm the connection state / type of the communication cable and the USB driver installation condition.
2. When using Ethernet cable, cancel the firewall setting of PC.

SYS00017

Creation of the %s folder failed during the %s process.

1. Release the lock switch of the SD card.
2. When using a model that can set write filter (write protection), remove the setting.

SYS00019

Data reception failed during the %s process.

SYS00032

The runtime was restarted. An unexpected error occurred.

An unexpected error occurred.

SYS00033

Changing Date/Time requires administrator rights.

You are not logged in with administrator rights.

Log in with a user set up with administrator rights.

SYS00034

Unable to export to the specified destination folder.

Invalid destination folder or you may not have administrator rights to use the specified folder.

Enter a valid destination folder or launch the application with the "Run as Administrator" option.

SYS00036

Transfer from external storage requires administrator rights.

SYS00037

The system data is invalid. Transfer the project file again using the file system transfer method.

Transfer the project file again using the file system transfer method.
Transferring a Project with the File System

SYS00050

Received a packet that is longer than expected.

Possible causes for this error include: protocol mismatch, network issues leading to corrupted packets, issues with buffer configuration, faulty equipment, malicious activities, and so on.

Review the network traffic, relevant server/client MTU configurations, and error logs.

SYS00051

The number of connections exceeded the limit.

Possible causes for this error include defective client applications and malicious activity, and so on.

Review the network connection, relevant server/client MTU configurations, and error logs.

SYS00101

The time variable value is invalid or has reached the maximum limit due to the passage of time. The variable value is reset to %s

The display unit clock data has been initialized.

Confirm the influence on functions using clock data and set the time of the display unit again.

SYS00102

Failed to overwrite the file (%s).

The file in external storage already exists and is either read-only or in use.

Check if the file is read-only and verify the file name.

SYS00201

Invalid user name or password. Type the user name and password again.

Enter a valid user name and password.

SYS01001

Duplicated IP address.

Please change the IP adress.

SYS02001

Charge the backup battery.

Rechargeable battery has run out of power.

Supply power to the display unit and fully charge the battery. In 24 hours the battery charges to a level that allows backup operation. Completing a full charge requires about 120 hours (5 days).

SYS02002

Replace the backup battery.
*1

Backup battery power is low.

_

SYS02003

The data in the backup memory (SRAM) has been deleted.
*1

Backup battery has run out of power.

SYS02004

Clock data has been initialized.
*1

The clock data has been deleted due to run out of battery power.

SYS03001

Calibration data has been initialized.

Calibration data is missing or broken.

Execute the calibration if necessary.

SYS03011

AlarmDB does not exist in %s.
(%s: SDCard/USBStorage/Internal)

-Check if the external storage is connected. If connected, disconnect and then reconnect the external storage.
-Transfer the project file again.

SYS03012

AlarmDefinitionDB does not exist in %s.
(%s: SDCard/USBStorage/Internal)

SYS03013

DataLoggingDB does not exist in %s.
(%s: SDCard/USBStorage/Internal)

SYS03014

RecipeDB does not exist in %s.
(%s: SDCard/USBStorage/Internal)

SYS03015

Japanese dictionary does not exist in %s.
(%s: SDCard/USBStorage/Internal)

SYS03016

OperationLogDB does not exist in %s.
(%s: SDCard/USBStorage/Internal)

SYS03017

The database is unavailable.

Due to an update to the run time, the used database signature algorithm is no longer supported.

Transfer the project file again to update the database signature algorithm.

COM00006

%s:%s Received data has been parity error
*1

An error occurred due to a lack of data received. The cause could be noise or poor connections.

Please check the noise suppression and connector's insertion. If Memory-Link method is used, please check if the Data Length/Parity Bit of host side and the display unit side have the same settings.

COM00007

%s:%s Received data has been framing error
*1

Please check the noise suppression and whether the connector is inserted properly.
If Memory-Link method is used, please check if the Data Length/Parity Bit on the host side and display unit side have the same settings.

COM00008

%s:This machine does not have any Ethernet interface

An error occurred when a Ethernet driver is selected in BLUE as the [System Configuration], but the project is transferred to the display unit which cannot use Ethernet.

Please check if the display unit supports Ethernet. If it does, please check if the Target settings in the BLUE editor are correct.

COM00009

%s:%s Cannot use the port

An error occurred when two or more driver types are selected to an identical COM port.

Please check the [Port] settings in BLUE [System Configuration].

COM00010

%s:TCP port number (%d) is overlapped, or it is not completed to close the last TCP connection
*1

TCP port number of the display unit side is overlapped, or the device/PLC is reset during communication.

(1) Check that the TCP port number in [Driver Configuration] does not overlap with the TCP port number in [Protocol Configuration]. If the TCP port number is overlapped, allocate a different port number.
(2) Reset the display unit.

COM00011

%s:Connection was closed
*1

An error occurred in the connection environment during communication.

Please check if the network environment is normal. Please specify the cause via procedures such as directly connecting PC, display unit and device/PLC, and then checking if IP address is recognized via PING command.

COM00012

%s:UDP port number is overlapped (%d)
*1

An error occurred when UDP port number of the display unit side is overlapped.

Check that the UDP port number in [Driver Configuration] does not overlap with the UDP port number in [Protocol Configuration]. If the UDP port number is overlapped, allocate a different port number.

COM00013

%s:%s:The 9th pin has not been set to VCC (5V Power Supply).Please check your cable or connected equipment
*1

9th pin of COM1 is connected as RI input. (For example, set to use Isolation Unit (RS-232C Type))

Please designate [RI] in [RI/VCC] settings of BLUE [System Configuration].

COM00014

%s:Memory link type drivers cannot be used at the same time
*1

This error appears if the Memory Link driver and a memory link type driver are used simultaneously.

COM00033

%s:Error has been responded for initial communication command (Error Code: %d[%XH])
*1

Device/PLC is returning an error code on a communication request from the display unit.

Please check the device/PLC manual for details on receive error codes.

COM00034

%s:Error has been responded for device read command (Error Code: %d[%XH])
*1

Device/PLC is returning an error code on a read request from the display unit.

Please check the device/PLC manual for details on error codes.

COM00035

%s:Error has been responded for device write command (Error Code: %d[%XH])
*1

Device/PLC is returning an error code on a write request from the display unit.

COM00036

%s:Error has been responded for device read command (Error Code: %d[%XH] There are out of range devices)
*1

Device/PLC cannot recognize the Read request of the address set via the display unit side, and return the error code. It might be set to request the address which is out of PLC address range on the display unit side.

(1) Please check the manual of device/PLC in use for the detail of receiving error codes.
(2) Please check if the address set is within the device/PLC device address range in use. If the error occurred in all screens, please check the addresses set via functions which operate in all screens, such as Alarm and Data Logging (Trend Graph). To check the addresses, from BLUE [Dashboard] view, select [Variable]. If the error occurred on specific screens, check the addresses for parts and functions that operate only on those specific screens.

COM00037

%s:Error has been responded for device write command (Error Code: %d[%XH] There are out of range devices)
*1

The Device/PLC cannot recognize the Write request of the address set on the display unit side, and returns the error code. It might be set to request an address which is out of the PLC address range on the display unit side.

(1) Please check the manual of device/PLC in use for the detail of receiving error codes.
(2) Please check if the address set is within the device/PLC device address range in use. If the error occurred in all screens, please check the addresses set via functions which operate in all screens, such as Alarm and Data Logging (Trend
Graph). To check the addresses, from BLUE [Dashboard] view, select [Variable]. If the error occurred on specific screens, check the addresses for parts and functions that operate only on those specific screens.

COM00038

%s:Error has been responded for device read command (Error Code: %d[%XH] There are write only devices)
*1

Device/PLC cannot recognize the Read request of the address set via the display unit side, and return the error code. It might be set to request the write only address of device/PLC on the display unit side.

(1) Please check the manual of device/PLC in use for the detail of receiving error codes.
(2) Please check if the address is set to read the write only address. *1
If Parts that perform reading operation such as Lamps and Data Display are used, please set to a read-only address.
*1 If the error occurred in all screens, please check the addresses set via functions which operate in all screens, such as Alarm and Data Logging (Trend Graph). To check the addresses, from BLUE [Dashboard] view, select [Variable]. If the error occurred on specific screens, check the addresses for parts and functions that operate only on those specific screens.

COM00039

%s:Error has been responded for device write command (Error Code: %d[%XH] There are read only devices)
*1

The Device/PLC cannot recognize the Write request of the address set on the display unit side, and returns the error code. It might be set to request the read only address of device/PLC on the display unit side.

(1) Please check the manual of device/PLC in use for the detail of receiving error codes.
(2) Please check if the address is set to write to the read-only address. *1
If Parts that perform writing operations, such as Switches, Data Displays (Allow Input) or Trigger Actions, are used, please change to read/write address.
*1 If the error occurred in all screens, please check the addresses set via functions which operate in all screens, such as Alarm and Data Logging (Trend Graph). To check the addresses, from BLUE [Dashboard] view, select [Variable].
If the error occurred on specific screens, check the addresses for parts and functions that operate only on those specific screens.

COM00040

%s:Illegal response for initial communication command
*1

An error occurred on device/PLC side.

Please check that the communication settings or the connected device settings are specified properly.

COM00041

%s:Illegal response for device read command
*1

Please check the communication settings and the connected device settings are specified properly.

COM00042

%s:Illegal response for device write command
*1

COM00043

%s:Checksum error response for initial communication command
*1

COM00044

%s:Checksum error response for device read command
*1

COM00045

%s:Checksum error response for device write command
*1

COM00049

%s:Unknown devices exist in read devices
*1

Wrong device and address are created via Indirect Address Designation.

Please check if settings of Indirect Address Designation are within the recognizable address range.

COM00050

%s:Unknown devices exist in write devices
*1

COM00051

%s:Out of range devices exist in read devices (Address:%s)
*1

In the Data Display (String Display), area from the start address to the end address is not within the address range.

Please check if the settings which is across multiple addresses, such as Data Display (String Display), are within the address range. If the error occurred in all screens, please check the addresses set via functions which operate in all screens, such as Alarm and Data Logging (Trend Graph). To check the addresses, from BLUE [Dashboard] view, select [Variable]. If the error occurred on specific screens, check the addresses for parts and functions that operate only on those specific screens.

COM00052

%s:Out of range devices exist in write devices (Address:%s)
*1

COM00053

%s:You cannot read the write only device (Address:%s)
*1

The Protocol driver detected read-out of the write only device, or write-in of the read only device.

(1) Please check the manual of device/PLC in use for the detail of receiving errorcodes.
(2) Please check if the address is set to read the write only address. If Parts that perform reading operation such as Lamps and Data Display are used, please set the read address.

COM00054

%s:You cannot write the read only device (Address:%s)
*1

COM00055

%s:Unknown variable address or tag name %s on the device
*1

This error appears when the Tag used in Device Address of the variable is not present in External Device.

Update the tag in Device Address.

COM00056

%s:Size of %s is not consistent with PLC symbol is referring to (expected: %d bytes)
*1

This error appears when there is diffrence in size of the tag used in Device Address of the variable and the external device. For example, If STRING size is different between the Variable and External Device.

(1) Update the variable or External Device.
(2) Update the variable and re-transfer the project to the External Device.

COM00057

%s:Type of %s is not consistent with PLC symbol is referring to
*1

This error appears when there is diffrence in data type of the tag used in Device Address of the variable and the external device. For example, If the variable has data type BYTE where as External Device has DWORD.

COM00065

%s:TCP connection open error (IP Address:%d.%d.%d.%d)
*1

IP address and port number of device/PLC are not recognized. The cause could be that the power of HUB or device/PLC is not ON, or cable is unplugged.

(1) Please check the settings of IP address and Port number on display unit side and device/PLC side.
(2) Please check if the network environment is normal. Please specify the cause via procedures such as directly connecting PC, display unit and device/PLC, and then checking if IP address is recognized via PING command.

COM00066

%s:UDP target not found (IP Address:%d.%d.%d.%d)
*1

COM00067

%s:Response timed out for initial communication command
*1

The causes could be the following:
1.The communication settings are not the same between display unit and PLC.
2.Wiring has problems such as a wrong wire connection or poor connection.
3.Selection of device/PLC is wrong.
4.The power of device/PLC is not ON, or it is reset.

(1) Please check if the communication settings of display unit side and device/PLC side are the same. Please refer to "Device/PLC Connection Manual" for the details.
(2) Please reconfirm the wiring. Please check the cable and connector's insertion.
About wire connection, please refer to "Device/PLC Connection Manual" for the details.
(3) Please reconfirm the BLUE [System Configuration].

COM00068

%s:Response timed out for device read command
*1

The causes could be the following:
1.The communication settings are not the same between display unit and PLC.
2.Wiring has problems such as a wrong wire connection or poor connection.
3.Selection of device/PLC is wrong.
4.The power of device/PLC is not ON, or it is reset.

COM00069

%s:Response timed out for device write command
*1

COM00070

%s:The cable has been disconnected or the target has been powered off
*1

The command cannot be sent due to the cause that the device/PLC power is not ON or cable is unplugged, etc.

(1) Check if the Target settings match the display unit model in use.
(2) Please check if the device/PLC power is ON.
(3) Please check if the cable wiring is correct, and if cable is connected properly.

COM00071

%s:The extend unit (%s) is not implemented

The Expansion Unit is not recognized.

Please check if the Expansion Unit is correctly attached.

COM00072

%s:Illegal read request because this device has been off scan

Sent a read request to a device/PLC that has communication turned off.

Turn on the device/PLC communication.

COM00073

%s:Illegal write request because this device has been off scan

Sent a write request to a device/PLC that has its communication turned off.

COM00076

%s: Requested device address (%s) does not exist on connected equipment.
*1

The connected equipment does not support the requested device address.

Please check the Device/PLC Connection Manual for supported device addresses, and in the screen editing software, change the device address.
To change the device address, in the [Project Explorer] window, go to [Variables] and click [All Variables]. Find the variable with the unsupported device address and change the address in the [Device Address] field.

COM00084

%s:Too many requests to write. The request was ignored
*1

A write operation was continued at timing which exceeds the processing speed of the communication driver.

Check if a setting has been specified which continues writing at fast speed.

COM00085

%s:Too many requests to read. The request was ignored
*1

A read operation was continued at timing which exceeds the processing speed of the communication driver.

Check if a setting has been specified which continues reading at fast speed.

COM00119

File is corrupted during transfer. Download the project file again.
*1

File is corrupted during transfer.

Download the project file to the display unit again.

COM00120

Settings are corrupted during transfer. Download the project file again.
*1

Settings are corrupted during transfer.

COM00121

Unable to access a driver.
*1

(1)Download the project file to the display unit again.
(2)Install the screen editor software again.

COM00128

"Equipment Name":No symbols are available or symbol mismatch
*1

CoDeSys Automation Alliance - CoDeSys V2 Ethernet

Register symbols that are used to the external device.

CoDeSys Automation Alliance - CoDeSys V3 Ethernet

COM00129

%s:[Equipment Security] does not match the PLC. Confirm the user name, password and encrypted communication.
*1

Enter a valid user name, password, and encrypted communication.

%s:Error has been responded for initial communication command(Error Code:[0x%X] Not implement(Robot Controller))
*1

DENSO WAVE INCORPORATED - b-CAP Protocol

Check the External Device type and version.

%s:Error has been responded for initial communication command(Error Code:[0x%X] Function abort(Robot Controller))
*1

Check the External Device program.

COM00130

%s:Error has been responded for initial communication command(Error Code:[0x%X] Function fail(Robot Controller))
*1

COM00131

%s:Error has been responded for initial communication command(Error Code:[0x%X] Fatal error(Robot Controller))
*1

COM00132

%s:Error has been responded for initial communication command(Error Code:[0x%X] Invalid recieve packet(Robot Controller))
*1

The External Device received a packet with invalid data. When this error occurs, the External Device automatically breaks the connection. Confirm the content of packets sent to the External Device.

COM00133

%s:Error has been responded for initial communication command(Error Code:[0x%X] Invalid send packet(Robot Controller))
*1

Please contact your local distributor.

COM00134

%s:Error has been responded for initial communication command(Error Code:[0x%X] Invalid argument type(Robot Controller))
*1

COM00135

%s:Error has been responded for initial communication command(Error Code:[0x%X] Robot is busy(Robot Controller))
*1

Check the operation end and run the PSTR.

COM00136

%s:Error has been responded for initial communication command(Error Code:[0x%X] Invalid command(Robot Controller))
*1

COM00137

%s:Error has been responded for initial communication command(Error Code:[0x%X] Packet size over(Robot Controller))
*1

COM00138

%s:Error has been responded for initial communication command(Error Code:[0x%X] Argument size over(Robot Controller))
*1

COM00139

%s:Error has been responded for initial communication command(Error Code:[0x%X] Access denied(Robot Controller))
*1

When occurs in PSTR, the Display unit's IP address is not registered in the controller's startup authority IP.

COM00140

%s:Error has been responded for initial communication command(Error Code:[0x%X] Illegal handle(Robot Controller))
*1

Address may be outside the supported address range. Check the device address.

COM00142

%s:Error has been responded for initial communication command(Error Code:[0x%X] Invalid argument(Robot Controller))
*1

Data written to a write disabled address.

COM00143

%s:Error has been responded for initial communication command(Error Code:[0x%X] Unknown Error(Robot Controller))
*1

Unknown error. ([0x????????] is undefined)

COM00144

%s:Shutdown... (Code:[0x%X])
*1

REBOOT device has been run.

COM00145

%s:It was not possible to execute it by out of range data
*1

Out of range data was written to DEVH, MOVE, DRAW, DRIVEEX devices.

COM00146

%s:Error has been responded for device read command(Error Code:[0x%X] Not implement(Robot Controller))
*1

COM00147

%s:Error has been responded for device read command(Error Code:[0x%X] Function abort(Robot Controller))
*1

COM00148

%s:Error has been responded for device read command(Error Code:[0x%X] Function fail(Robot Controller))
*1

COM00149

%s:Error has been responded for device read command(Error Code:[0x%X] Fatal error(Robot Controller))
*1

COM00150

%s:Error has been responded for device read command(Error Code:[0x%X] Invalid recieve packet(Robot Controller))
*1

The External Device received a packet with invalid data. When this error occurs,
the External Device automatically breaks the connection. Confirm the content of packets sent to the External Device.

COM00151

%s:Error has been responded for device read command(Error Code:[0x%X] Invalid send packet(Robot Controller))
*1

COM00152

%s:Error has been responded for device read command(Error Code:[0x%X] Invalid argument type(Robot Controller))
*1

COM00153

%s:Error has been responded for device read command(Error Code:[0x%X] Robot is busy(Robot Controller))
*1

Confirm the operation has ended, then run PSTR.

COM00154

%s:Error has been responded for device read command(Error Code:[0x%X] Invalid command(Robot Controller))
*1

COM00155

%s:Error has been responded for device read command(Error Code:[0x%X] Packet size over(Robot Controller))
*1

COM00156

%s:Error has been responded for device read command(Error Code:[0x%X] Argument size over(Robot Controller)
*1

COM00157

%s:Error has been responded for device read command(Error Code:[0x%X] Access denied(Robot Controller))
*1

COM00158

%s:Error has been responded for device read command(Error Code:[0x%X] Illegal handle(Robot Controller))
*1

COM00160

%s:Error has been responded for device read command(Error Code:[0x%X] Invalid argument(Robot Controller))
*1

COM00161

%s:Error has been responded for device read command(Error Code:[0x%X] Unknown Error(Robot Controller))
*1

COM00162

%s:Error has been responded for device write command(Error Code:[0x%X] Not implement(Robot Controller))
*1

COM00163

%s:Error has been responded for device write command(Error Code:[0x%X] Function abort(Robot Controller))
*1

COM00164

%s:Error has been responded for device write command(Error Code:[0x%X] Function fail(Robot Controller))
*1

COM00165

%s:Error has been responded for device write command(Error Code:[0x%X] Fatal error(Robot Controller))
*1

COM00166

%s:Error has been responded for device write command(Error Code:[0x%X] Invalid recieve packet(Robot Controller))
*1

COM00167

%s:Error has been responded for device write command(Error Code:[0x%X] Invalid send packet(Robot Controller))
*1

COM00168

%s:Error has been responded for device write command(Error Code:[0x%X] Invalid argument type(Robot Controller))
*1

COM00169

%s:Error has been responded for device write command(Error Code:[0x%X] Robot is busy(Robot Controller))
*1

COM00170

%s:Error has been responded for device write command(Error Code:[0x%X] Invalid command(Robot Controller))
*1

COM00171

%s:Error has been responded for device write command(Error Code:[0x%X] Packet size over(Robot Controller))
*1

COM00172

%s:Error has been responded for device write command(Error Code:[0x%X] Argument size over(Robot Controller))
*1

COM00173

%s:Error has been responded for device write command(Error Code:[0x%X] Access denied(Robot Controller))
*1

COM00174

%s:Error has been responded for device write command(Error Code:[0x%X] Illegal handle(Robot Controller))
*1

COM00176

%s:Error has been responded for device write command(Error Code:[0x%X] Invalid argument(Robot Controller))
*1

Data written to write disabled address.

COM00177

%s:Error has been responded for device write command(Error Code:[0x%X] Unknown Error(Robot Controller))
*1

Memory Link:Checksum does not match the data actually received(ErrorCode:%02X Destination:%s)
*1

Pro-face by Schneider Electric - Memory Link SIO

The check sum is wrong in the sending sentence. Correct the sending sentence.

Memory Link:Undefined code has been recived(ErrorCode:%02X Destination:%s)
*1

The command in the sending sentence is wrong. Correct the sending sentence.

Memory Link:The specified number of data elements does not match the number of data elements received(ErrorCode:%02X Destination:%s)
*1

The number of data elements in the sending sentence is wrong. Correct the sending sentence.

Memory Link:The specified address in the system area is out of the permissible range(ErrorCode:%02X Destination:%s)
*1

The system area specification in the sending sentence is wrong. Correct the sending sentence.

Memory Link:An attempt has been made to write to or read from outside the system area(ErrorCode:%02X Destination:%s)
*1

Exceeded the system area range. Correct the sending sentence.

Memory Link:A data block of an improper format has been received by the AGP(ErrorCode:%02X Destination:%s)
*1

The format in the sending sentence is wrong. Correct the sending sentence.

Memory Link:The AGP has been unable to send data(ErrorCode:%02X Destination:%s)
*1

The Display unit cannot send the command. Check the cable wiring

%s:PLC returned error code. ([%02d]:[%02d])
*1

Emerson Process Management - ROC Plus Series Ethernet

General error code

%s:PLC returned error code. ([%02d]Data bytes too many)
*1

Too many data bytes

%s:PLC returned error code. ([%02d]Data byte too few)
*1

Too few data bytes

%s:PLC returned error code. ([%02d]Invalid Parameter Range)
*1

Invalid parameter range

%s:PLC returned error code. ([%02d]Invalid Min/Max Request)
*1

Invalid min/max request

%s:PLC returned error code. ([%02d]Invalid Time)
*1

Invalid time

%s:PLC returned error code. ([%02d]:[%02d]Unknown Error)
*1

Unknown error

%s:PLC returned error code. (Invalid Parameter Number (%s))
*1

Invalid parameter number

%s:PLC returned error code. (Invalid Logical/Point Number (%s))
*1

Invalid logical/point number

%s:PLC returned error code. (Invalid Type Number (%s))
*1

Invalid type number

Emerson Process Management - ROC Plus Series SIO

%s:Error has been responded for device read command (Major:[%02XH], Minor:[%02XH])
*1

FANUC LTD. - Power Mate Series

Error has been responded for device read command.

%s:Error has been responded for device write command (Major:[%02XH], Minor:[%02XH])
*1

Error has been responded for device write command.

%s:The specified destination module number does not exist.(Error Code:[%02XH])
*1

Fuji Electric Co., Ltd. - MICREX-SX Series Ethernet

It occurs when accessing a non-existing CPU No., and SX No. Designate existing module.

GE Intelligent Platforms - Series 90 Ethernet

Displayed when error occurs by device read command.

Displayed when error occurs by device write command.

%s:Unsupported devices exist in read devices
*1

Displayed when trying to read "%W" device for External Device except RX7i.

%s:Unsupported devices exist in write devices
*1

Displayed when trying to write "%W" device for External Device except RX7i.

%s:It was not possible to execute it by out of range data.

IAI Corporation - X-SEL Controller

Data write beyond the data range was requested.

%s:PC2 mode is not supported.
*1

JTEKT Corporation - TOYOPUC CMP-LINK Ethernet

PC2 mode is not supported.

%s:%s device is not supported in PC3 Mode
*1

The specified device is not supported in PC3 mode.

%s:Out of range device in PC3 Mode(Address:%s)
*1

The specified device address is out of the supported range in PC3 mode.

%s:The setting value for Watch Time Register is illegal.
*1

The setting value may be illegal. Check the device value.

%s:it failed in the writing mode setting.
*1

JTEKT Corporation - TOYOPUC CMP-LINK SIO

Please check the connection.

%s:AGP cannot read or write when "I/O No." and "Station No." are set.
*1

Mitsubishi Electric Corporation - Q/QnA Series Ethernet

When both "I/O No." and "Station No." in "Request destination module" are set and then access is made to other station, the display unit reads or writes data to the Control CPU only in Multiple CPU system.

%s:The specified CPU in the Device Address exceeded the set value of Multiple CPU System. (Address:%s)
*1

The specified CPU No.1 for read or write does not exist.

The specified CPU No.2 for read or write does not exist.

The specified CPU No.3 for read or write does not exist.

The specified CPU No.4 for read or write does not exist.

%s:The specified CPU unit could not be accessed. (Address:%s)
*1

Mitsubishi Electric Corporation - Q Series QnU CPU Ethernet

Appears if you access a CPU number that is not assigned.

%s:The specified password is incorrect (Error Code:[%04XH]).
*1

Mitsubishi Electric Corporation - iQ-R/F Series Ethernet

Unable to unlock because the password is incorrect.

%s:Remote Password: Illegal Format.
*1

Invalid password format.

%s: %s is not defined on Function Code and Max Query setting
*1

Modbus Organization - Modbus SIO ASCII Master

When accessing the device out of the defined area, an error will be displayed.

%s: %s can't be read because of the limitation of the Device Range setting
*1

When reading the coil or discrete input as a word address while the range is less than 16 bits, or accessing the input or holding register as a double word while the range is set to 1 word, an error will be displayed.

%s: %s can't be written because of the limitation of the Device Range setting
*1

When writing the coil as a word address while the range is less than 16 bits, or accessing the holding register as a double word while the range is set to 1 word, an error will be displayed.

Modbus Organization - Modbus SIO Master

Modbus Organization - Modbus TCP Master

%s:Error has been responded for device read command (Main Response:[%02XH], Sub Response:[%02XH])
*1

OMRON Corporation - CS/CJ Series Ethernet

Display the error message, when the error occurred by the reading demand.

%s:Error has been responded for device write command (Main Response:[%02XH], Sub Response:[%02XH])
*1

Display the error message, when the error occurred by the write demand.

OMRON Corporation - CS/CJ Series HOST Link

%s:Error has been responded for initial communication command (Encapsulation Error Code:[%08XH])
*1

OMRON Corporation - CS/CJ/NJ Series Ethernet/IP

Error has been responded for initial communication command.

%s:Error has been responded for device read command (Encapsulation Error Code:[%08XH])
*1

%s:Error has been responded for device write command (Encapsulation Error Code:[%08XH])
*1

%s:Error has been responded for initial communication command (CIP Error Code:[%02XH])
*1

%s:Error has been responded for device read command (CIP Error Code:[%02XH])
*1

%s:Error has been responded for device write command (CIP Error Code:[%02XH])
*1

%s:Error has been responded for initial communication command (General STS Code:[%02XH], Additional STS Code:[%04XH])
*1

%s:Error has been responded for device read command (General STS Code:[%02XH], Additional STS Code:[%04XH])
*1

%s:Error has been responded for device write command (General STS Code:[%02XH], Additional STS Code:[%04XH])
*1

%s:To get the tag information failed (The tag counts which failed to get:[%d])
*1

Received from the External Device an error response to the get address packet. On the External Device, register the tags you are accessing from the display unit.

%s:Internal Error [%XH,%XH,%u]
*1

Displayed when error occurs by device internal error.

COM00141

%s:Initial communication failed (CIP Error Code:[%02XH,%XH,%u])
*1

Displayed when error occurs by device initial command.

%s:Device read failed (CIP Error Code:[%02XH,%XH,%u])
*1

%s:Device write failed (CIP Error Code:[%02XH,%XH,%u])
*1

%s:Initial communication failed (Error Code:[%XH,%u])
*1

%s:Device read failed (Error Code:[%XH,%u])
*1

%s:Device write failed (Error Code:[%XH,%u])
*1

%s:USB storage location not found.
*1

USB storage is not connected. Check the USB storage device.

%s:SD card access error (Error Status:[%d])
*1

Unable to access the SD card Check the SD Card. Error status
1: SD card is not inserted.
2: Unmount
3: Unformatted
4: Write-protect 5: Others

%s:Error has been responded for device read command (STS Response:[%02XH], EXT Response:[%02XH])
*1

Rockwell Automation, Inc. - DF1

%s:Error has been responded for device write command (STS Response:[%02XH], EXT Response:[%02XH])
*1

A Station with the same ID as the Source ID was detected(Station ID:%d)
*1

Rockwell Automation, Inc. - DH-485

Duplicate ID was detected.

A Station with an ID greater than the Maximum ID was detected(Maximum ID:%d)
*1

Illegal ID was detected.

An error response has been received from the External Device for a read command.

An error response has been received from the External Device for a write command.

DH-485 driver can not be used with COM1 and COM2 at the same time
*1

DH-485 driver can not be used with COM1 and COM2 at the same time.

The driver(in COM%d) can not be used together with DH-485
*1

The driver(in COM%d) can not be used together with DH-485.

Rockwell Automation, Inc. - EtherNet/IP

%s:Error has been responded for device read command (Error Code:[STS Code:%02XH][EXT Code:%02XH])
*1

%s:Error has been responded for device write command (Error Code:[STS Code:%02XH][EXT Code:%02XH])
*1

%s:The Input data is out of range(Address:(%s))
*1

Sanmei Electronics Co., Ltd. - Si/CutyAxis Series SIO

As for device PT, PNT, if the set value is out of the range, the error will display.

%s:During servo-on, an attempt was made to execute the command [RESET] (CPU reset)
*1

Execute the RESET command during servo ON, the error will display.

Schneider Electric - PacDrive

Schneider Electric - Machine Expert Network

Mpi connection is not supported.
*1

Siemens AG - SIMATIC S7 MPI Direct

Your setup environment does not support MPI communication. Refer to the Device/PLC Communication Manual for the setup environments you can use for MPI communication, and adjust your system configuration accordingly.

Illegal Highest Node
*1

The Highest MPI Address is illegal. Change it to 15/31/63 or 126 numbers.

Illegal Node address.
*1

A MPI Node exists that exceeds the Highest MPI Address. Fix the MPI Node number of Highest MPI Address.

Duplicate node found in MPI network.
*1

A duplicated MPI Node has been detected on the network. Reassign the node numbers.

Target Node Not Found (%s)
*1

The requested target node is not in the token ring. Verify that the target node number is correct and that the target is connected to the network.

MPI network error.
*1

The display unit does not detect the presence of the token ring. Check Baud Rate settings and cable etc..

%s:Error has been responded for device read command (Error Code: [%X])
*1

Siemens AG - TIA Portal Ethernet

%s:Error has been responded for device write command (Error Code: [%X])
*1

%s:Invalid password. Type the password again.
*1

The specified password does not match the password in the TIA Portal project file. Please set the correct password.

%s:Password is not configured on the PLC. In [Equipment Security], remove the password.
*1

In [Equipment Security], remove the password.

Password is configured on the PLC. In [Equipment Security], set up the corresponding password.
*1

In [Equipment Security], set up the corresponding password.

%s:Error has been responded for device read command (General status:[%02XH], Extended status:[%02XH])
*1

YASKAWA Electric Corporation - High Speed Ethernet Server

Error status received from the device on a load command.

%s:Error has been responded for device write command (General status:[%02XH], Extended status:[%02XH])
*1

Error status received from the device on a write command.

%s:PLC is busy now(Error Code:[%02XH])
*1

YASKAWA Electric Corporation - MP Extension SIO

PLC is "Busy"

%s:Option module is not mounted(Error Code:[%02XH])
*1

Option module not mount.

%s:Module is not ready(Error Code:[%02XH])
*1

Module is not ready.

%s:CPU is stopped(Error Code:[%02XH])
*1

CPU is stopped.

%s:Write protected(Error Code:[%02XH])
*1

Write protected.

YASKAWA Electric Corporation - MP Ethernet/MECHATROLINK

PLC is "Busy". For an error code is refer to Error Code list.

Option module not mount. For an error code is refer to Error Code list.

Module is not ready. For an error code is refer to Error Code list.

CPU is stopped. For an error code is refer to Error Code list.

Write protected. For an error code is refer to Error Code list.

%s:Error has been responded for device read command (Error Code:[%02XH,%02XH])
*1

The error message is displayed when the error has occurred in the read command. For an error code is refer to Error Code list.

%s:Error has been responded for device write command (Error Code:[%02XH,%02XH])
*1

The error message is displayed when the error has occurred in the write command. For an error code is refer to Error Code list.

%s:Error has been responded for device read command (Error Code:[%02XH,%02XH,%02XH])
*1

%s:Error has been responded for device write command (Error Code:[%02XH,%02XH,%02XH])
*1

%s:Error has been responded for device read command (Error Code:[%02XH,%02XH,%02XH] There are out of range devices)
*1

%s:Error has been responded for device write command (Error Code:[%02XH,%02XH,%02XH] There are out of range devices)
*1