# Error Code

### MP Series

Error Code | Description
0x90 | Transfer error
0x92 | Illegal parameter
0x96 | Register No. over
0x9C | File is modified
0x9D | Data access error

### Inverter Series

Error Code | Description
0x01 | Function code error
0x02 | Invalid register number error
0x03 | Invalid quantity error
0x21 | Data setting error
0x22 | Write mode error
0x23 | Main circuit undervoltage (UV) error during write
0x24 | Write error during processing of constants

### Servo Series

Error Code | Description
0x01 | Function Code Error Unsupported function code or sub function code in use.
0x02 | Faulty Register Number Accessing register number that is not registered.
0x03 | Faulty Quantity The number of read or write data for reading is not between one and the maximum quantity (as defined per model). In write mode, the number of data in the message is not the specified quantity.
0x30 | Faulty Register Number (High Level) Accessing register number that is not registered.
0x31 | Access Limit Error Access to the specified register is not permitted.
0x32 | Outside Setting Range Error The write data value is outside the maximum and minimum limit.
0x33 | Data Matching Error Tried to access only a portion of registers in the multiple register unit. Tried to access multiple registers that exceed the register group.
0x34 | Condition Error Command message content cannot be processed due to the condition defined by the register.
0x35 | Process Conflict Error Cannot be processed due to priority issues with other channels.
0x36 | Axis number error (Σ-7W/Σ-7C series only) The extended address is using an axis number that is not available.

### I/O (M-System)

Error Code | Description
0x01 | Function Code Error Unsupported function code or sub function code in use.
0x03 | Faulty Quantity The data count in read or write operations is outside the allowed range (1 to the maximum, as defined per model). In write mode, the data count in the message does not match the specified quantity.
0x04 | Data Type Error Not supported by the defined mode or data type.
0x09 | Process Conflict Error Cannot process due to priority issues with other channels.
0x81 | Protocol ID Setting Error When running a vendor specific command, the protocol ID did not match the I/O.
0x82 | Data Length Setting Error When running a vendor specific command, the data length setting for the vendor special area does not match the I/O.
0x83 | Vendor Special Area Error When running a vendor specific command, a vendor special error occurred in the vendor special area.

Example:

Error code = 0x83, and the vendor special error code = 0x01, it is displayed 83,01.

Vendor special error code

Error Code | Description
0x01 | Model code error The specified model code does not match the I/O.
0x02 | Specified channel error The I/O does not support the specified channel.
0x03 | Setting command error The I/O does not support the setting command.
0x04 | Setting command data error Error in the setting command data.

- If the error code is 0x83, it is displayed together with the vendor special error code.

### I/O (Azbil)

Error Code | Description
0x01 | Function Code Error Unsupported function code or sub function code in use.
0x02 | Memory Address Error Memory address you tried to access is not in the memory address range.
0x03 | Faulty Quantity The data count in read or write operations is outside the allowed range (1 to the maximum, as defined per model).
0x04 | Data Type Error Not supported by the defined mode or data type. Not supported by the protocol ID or device code.
0x81 | Protocol ID Setting Error When running a vendor specific command, the protocol ID did not match the I/O.
0x82 | Data Length Setting Error When running a vendor specific command, the data length setting for the vendor special area does not match the I/O.
0x83 | Vendor Special Area Error When running a vendor specific command, a vendor special error occurred in the vendor special area.

Vendor special error code

Error Code | Description
0x01 | Azbil protocol ID setting error The specified Azbil protocol ID is not supported by the I/O.

Example:

Error code = 0x83, vendor special error code = 0x81, and Modbus error code = 0x01, it is displayed 83,81,01.

Vendor special error code

Error Code | Description
0x81 | MODBUS RTU abnormal response Received a Modbus error. For more information, check the Modbus error code table.

Modbus error code

Error Code | Description
0x01 | Illegal function Unsupported function code in use Connected to unsupported the I/O
0x02 | Illegal data address Data address error (area where access is prohibited)
0x03 | Illegal data Write out-of-range value Equipment related, write-protected and read prohibited
0x13 | Write mode error

- If the error code is 0x83, and the vendor special error code is 0x01, it is displayed 83,01.
- If the error code is 0x83, and the vendor special error code is 0x81, it is displayed together with the Modbus error.

### Stepping (ORIENTAL MOTOR)

Error Code | Description
0x01 | Function Code Error Unsupported function code or sub function code in use.
0x02 | Faulty Register Number Accessing register number that is not registered.
0x03 | Faulty Quantity The number of read or write data for reading is not between one and the maximum quantity (as defined per model). In write mode, the number of data in the message is not the specified quantity.
0x04 | Data Type Error Not supported by the defined mode or data type.
0x05 | Access Limit Error Access to the specified register is not permitted.
0x06 | Outside Setting Range Error The write data value is outside the maximum and minimum limit.
0x07 | Data Matching Error Tried to access only a portion of memory in the multiple register unit. Tried to access multiple registers that exceed the register group.
0x08 | Condition Error Command message content cannot be processed due to the condition defined by the register.
0x09 | Process Conflict Error Cannot be processed due to priority issues with other channels.