# Exporting Logged Data

You can export the logged data into an external storage.

## Example Operation

## Setting Workflow

1. Add Variables
2. Add Logging Group
3. Assign the Variables
4. Set up Parts
5. Set up Scripts

## Add Variables

### Project Explorer : [Variables] ➞ [All Variables]

Add the following variables.

#### Variables properties :

[Name] | [Data Type] | [Source] | [Device Address]
Var1 | [INT] | 'Schneider Modbus Serial Equipment' | 400005
Var2 | [INT] | 400030
Var3 | [INT] | 400031
Var4 | [BOOL] | (Any) | (Any)

## Add Logging Group

### Project Explorer : [Logging] ➞ [All Loggings]

#### [All Loggings] properties :

Tab | Property | Value
[Basic] | [Max Record] | 300

### Project Explorer : [All Loggings]

Add the following logging group.

[Name]
LoggingGroup1

#### Logging Group (Name: LoggingGroup1) properties :

Tab | Property | Value
[Basic] | [Condition Type] | [ValueChange]
[Execution Condition] | [ON]
[Trigger Variable] | [Variable] [Name]: Var4
[Export Data] |
[Write Data To] | [USB Storage]
[Folder Name] | \LoggingGroup
[File Name] | LoggingGroup1

## Assign the Variables

### Project Explorer : [LoggingGroup1]

Assign the following variables.

#### Logging Group1 properties:

[Variable Name]
Var1
Var2
Var3

## Set up Parts

### Project Explorer : [Screen Design] ➞ [Screens] ➞ [Screen1]

Drag and drop the following objects from the [Tool Chest] to the screen.

#### Switch object (Name: Switch1) properties :

Default value.

## Set up Scripts

### Project Explorer : [Screen1]

Set the following script on the object.

From the [Tool Chest] drag and drop the script to the Script editor.

#### Switch object (Name: Switch1) script :

Legend | Block
1 | [Triggers] ➞ [Touch] ➞ [Touch]
2 | [Values] ➞ [Screen Object]
3 | [Operations] ➞ [HMI Functions] ➞ [Export Log Data]