### KV-3000/5000/5500 Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | R00000 - R99915 | R000 - R999 |  |
Output Relay |
Internal Auxiliary Relay |
Link Relay | B0000 - B3FFF | B000 - B3FF | *4
Internal Auxiliary Relay | MR00000 - MR99915 | MR000 - MR999 |
Latch Relay | LR00000 - LR99915 | LR000 - LR999 |
Control Relay | CR0000 - CR3915 | CR00 - CR39 |
Work Relay | VB0000 - VB3FFF | VB000 - VB3FF | *4
Timer (Contact) | T0000 - T3999 | ----- | - |
Counter (Contact) | C0000 - C3999 | ----- |
High-speed Counter Comparator (Contact) | CTC0 - CTC3 | ----- | *1
Timer (Setting Value) | ----- | TS0000 - TS3999 |  | *2
Counter (Setting Value) | ----- | CS0000 - CS3999 | *2
Timer (Current Value) | ----- | TC0000 - TC3999 | *2
Counter (Current Value) | ----- | CC0000 - CC3999 | *2
Data Memory | ----- | DM00000 - DM65534 |
Extension Data Memory | ----- | EM00000 - EM65534 |
File Register | Current Bank | ----- | FM00000 - FM32767 |
Serial Number System | ----- | ZF000000 - ZF131071 |
Temporary Data Memory | ----- | TM000 - TM511 |
Control Memory | ----- | CM00000 - CM05999 |
Link Register | ----- | W0000 - W3FFF |
Work Memory | ----- | VM00000 - VM59999 |
Index Register | ----- | Z01 - Z12 | *2 *3
Digital Trimmer | ----- | TRM0 - TRM7 | *1 *2
High-speed Counter (Current Value) | ----- | CTH0 - CTH1 | *2
High-speed Counter Comparator (Setting Value) | ----- | CTC0 - CTC3 | *2

*1Write disable

*232-bit device

*3Z11 and Z12, used by the External Device system, are not available to write in.

*4The word address descriptions used in the BLUE and the External Device are different. Please be aware of these differences when setting up word addresses.

BLUE | External Device
B000 - B3FF | B0000 - B3FF0
VB000 - VB3FF | VB0000 - VB3FF0

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms