Display (Connection Port) | Cable | Notes
--- | --- | ---
SP-5B10 (COM1/2) SP-5B90 (COM1/2) ST6000 (COM2)*b-3 ST-6200 (COM1) ST6000 2nd Gen*d-4 *d-5 (COM2) PFXST6200AWADI*d-4 (COM1) STM6000 (COM1) | 1A | MPI Cable (3.5m) by Pro-face ST03-A2B-MPI21-PFE*1 | The cable length have to be 50m or less in one segment.
SP5000 (Expansion Unit*2) SP5000X (Expansion Unit*2) | 1E | PROFIBUS compliant connector + PROFIBUS compliant cable*10 | The cable length have to be 50m or less in one segment.
1F | MPI Cable (3.5m) by Pro-face CA3-MPI-PGN-PFE or MPI Cable (3.5m) by Pro-face CA3-MPI-PG1-PFE | The cable length have to be 50m or less in one segment.

*1 There are Display side connector and the External Device side connector on the MPI cable (ST03-A2B-MPI21-PFE).
Check the Display side and the External Device side, and please connect correctly.
Reversing the cable connections between the Display side and External Device side may damage and ruin the CPU unit.

*2You need the PROFIBUS DP Slave/MPI Unit (PFXZCDEUPF1) by Pro-face.

*10Please be aware that certain PROFIBUS compliant cable have restriction on baudrate.

*b-3Except ST-6200

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

*d-5Except PFXST6200AWADI

IMPORTANT:

- Use a cable manufactured from Pro-face or a PROFIBUS compliant cable/connector for connecting with the External Device.
  If a user-created cable is used and cable connection is incorrect, the Display may be broken down.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.