### 10A

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) SIO connector side: D-Sub 9 pin (socket) |
(2) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(3) | Network Connection Cable by IAI Corporation CB-ERC2-CTL001 | Connect to the J4 or J5 on the SIO converter
(4) | Power & I/O Cable by IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB |

NOTE

- Cable length from Display to SIO converter: 15m or less

*1 We recommend the IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB as the Power & I/O Cable.