### 5K

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: Terminal block | Instead connecting the Display (FG), connect the Shield to the Shell.
(2) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB |

NOTE

- Cable length: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB as the Power & I/O Cable.