NOTE

- When use FP0H, select "FP Series" from [Series].

###

### External Device Settings

Use the programming software (FPWIN GR7) to set up communication settings on the External Device.

For details on communication settings, please refer to the manual of the External Device.

1. Select [Create a New Project] and click [OK].

2. From the [Select PLC Type] window select the Series and Model then click [OK].

3. From the project tree double click [Ethernet settings].

4. From the [Ethernet settings] window click [Basic communications information].

5. Set items to the following values.

   Setup Item | Setting description
   --- | ---
   IPv4 address automatic acquisition | No
   Home IP address | 192.168.1.5
   Subnet mask | 255.255.255.0

6. Click [OK].

7. From the [Ethernet settings] window click [Connection 1].

8. Set items to the following values.

   Setup Item | Setting description
   --- | ---
   Connection to use specification | Use
   Communication type | TCP/IP
   Open type (server/client) | Server connection (any destination)
   Open type (automatic/manual) | Open automatically
   Operating mode setting | MEWTOCOL-COM
   MEWTOCOL communications type | Not connect with FP2 ET-LAN
   Home port number | 60001
   Unused connection disconnect time | 0

9. Click [OK].

10. Download the project to the External Device.

11. Reboot the External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.