#### SPH200 (NP1PH-08)

Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input Memory | %IX□.000.00 - %IX□.511.15 | %IW□.000 - %IW□.511 |  | *1
Output Memory | %QX□.000.00 - %QX□.511.15 | %QW□.000 - %QW□.511 | *1
Standard Memory | %MX□.1.00000.00 - %MX□.1.04095.15 | %MW□.1.00000 - %MW□.1.04095 | *2 *3
Retain Memory | %MX□.3.0000.00 - %MX□.3.2047.15 | %MW□.3.0000 - %MW□.3.2047 | *2 *3
System Memory | %MX□.10.000.00 - %MX□.10.511.15 | %MW□.10.000 - %MW□.10.511 | *2

*1Input/Output Memory Address Designation is as shown below.

- Bit Designation

- Word Designation

NOTE

- Please Refer to the SX Bus Unit no. details in the manual of External Device.

*2Standard/Retain/System Memory Address Designation is as shown below.

- Bit Designation

- Word Designation

*3Standard and Retain Memory sizes can be changed. However, the total memory size is fixed. (For details, refer to the manual of External Device).

NOTE

- When specifying the address of the External Device directly, always use a setting within the specified AT range of the ladder software. We recommend using an AT-specified- variable for the External Device used on the Display. Please refer to the MICREX-SX Series D300Win <Reference> Users Manual by Fuji Electric Co., Ltd. for details of specifying the AT range and how to set it. When using a variable that is not AT-specified, variable needs to be imported again and screen transfer needs to be executed if ladder program or variable is changed.
- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms