### FP7 Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External input relay | X00000 - X0511F | WX0000 - WX0511 |  | *1
External output relay | Y00000 - Y0511F | WY0000 - WY0511 | *1
Internal relay | R00000 - R02047F | WR0000 - WR2047 | *1
Link relay | L00000 - L1023F | WL0000 - WL1023 | *1
System relay | SR00000 - SR0223F | WS0000 - WS0223 | *2
Timer(Contact) | T00000 - T04095 | -------- | *1 *2
Counter(Contact) | C00000 - C01023 | -------- | *1 *2
Pulse relay | P00000 - P0255F | -------- | *1 *2
Error alarm relay | E00000 - E04095 | -------- | *1 *2
Direct input | IN00000 - IN0062F | WI0000 - WI0062 | *2 *3
Direct output | OT00000 - OT0062F | WO0000 - WO0062 | *3
Data register | DT000000.0 - DT999423.F | DT000000 - DT999423 | *1 *6
Link register | LD00000.0 - LD16383.F | LD00000 - LD16383 | *1
Unit Memory | UM00000.0 - UM7FFFF.F | UM00000 - UM7FFFF | *3 *5
System data | -------- | SD00000 - SD00255 | *2
Timer set value register | -------- | TS00000 - TS04095 | *1 *4
Timer elapsed value register | -------- | TE00000 - TE04095 | *1 *4
Counter set value register | -------- | CS00000 - CS01023 | *1 *4
Counter elapsed value register | -------- | CE00000 - CE01023 | *1 *4
Index register | -------- | I0000 - I000E | *4 *5

*1You can use these devices as a global device and local device. If used as a local device, configure a program block number. Please enter the program block number of the program with the local device. Example: X000 (Global external input device, address 000) 023_X000 (Local external input device, Program block 23, address 000) *2Write disabled *3You need to set the slot number for these devices. You can use these devices without the program block number. Example: S16:IN000 (Direct input device, Slot number 16, address 000) *432-bit device *5Hexadecimal address *6Maximum address within one program block is 65533.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms