### Settings of External Device

Use the ladder software SX-Programmer Expert (D300win) for communication settings.

Please refer to the Micrex-SX Series D300Win users manual by Fuji Electric Co., Ltd. for more details.

1. Start up the D300win.

2. Select [New Project] from the [File] menu and select template of using CPU from the New Project dialog.

3. Double click [System Definition] of the project tree to display the system definition screen.

4. Select [Insert] from the displayed menu indicated after right-clicking the CPU.

5. Select Ethernet interface module to be used from [Outline Specification] of the displayed [Module insert] dialog box and register it to the system definition.

6. Right click Ethernet interface module and select [Properties] from the displayed menu.

7. Click [Parameter] of the [Module properties] dialog box.

8. Select [IP Address] tub of [Ethernet Parameter] dialog box.

9. Input IP address and subnet mask as shown below in [IP Address].

   Setup Items | Setup Description
   --- | ---
   IP Address | 192.168.0.1
   Subnet mask | 255.255.255.0

10. Select [Detail Setting] of [Ethernet Parameter] dialog box.

11. Select [Self port standard No.] and input "773" to the port number above Ethernet interface module.

NOTE

- For the port number of Device Setting for BLUE, set the value that "251" is added to the set port number.
  For example, if "773" is set to the port number, set "1024" to the port number of Device Setting for BLUE.

12. Select [Exit] from [File] menu on the system definition screen.

13. Select [Make] from [Build] menu and compile the project.

14. Select [Project Control] from [Online] menu and click [Download].

15. Select all items to be downloaded and click [OK].

16. After download is executed normally, click [Reset].

Now communication setting is completed.

NOTE

- When using a CPU other than the SPH5000M Series, in the driver properties, select [Other CPU] for the [CPU Series].
- In a multi-CPU configuration that includes the SPH5000M Series, even if there is no communication with SPH5000M Series, in the driver properties, select [SPH5000M] for the [CPU Series].