### Setting of External Device

Use the switches on the side of Ethernet module for setting the External Device.

##### IP Address Setting Switch

Use 8 Hex rotary switches for setting.

Setup Items | Setup Description
--- | ---
IP Address Setting Rotary Switch | Option

##### Port No.

Setup Items | Setup Description
--- | ---
Port No. | 12289

##### Condition Setting Switch

DIP Switch | Settings | Setup Description
--- | --- | ---
SW1 | OFF | ASCII
ON | Binary
SW2 | OFF | Not protect
SW3 | --- | (Reserved)
SW4 | --- | (Reserved)
SW5 | --- | (Reserved)
SW6 | --- | (Reserved)
SW7 Deleted "*1". (*1 SW7 is available to set in F3LE01-5T only.) Because, only users who are using "F3LE01-5T" see this page. | OFF | Close
SW8 | OFF | Normal

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.