### 3B

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display: side: Terminal Block External Device: Half pitch 14 pin | Connect the shield to FG (Shell).

NOTE

- We recommend following connector and case on the External Device side.
  Connector: HDR-E14MAG1+ by HONDA TSUSHIN KOGYO CO., LTD.
  Case: HDR-E14LPA5 by HONDA TSUSHIN KOGYO CO., LTD.
- Cable length: 30m or less.