Hide Show

1. Connection Configuration
2. Communication Settings
3. Cable Diagram
4. Supported Devices

1. Setting Items List

IMPORTANT:

- If problems such as communication interruptions due to a disconnection of the signal wire or malfunction of the Display cannot be detected on the inverter side, implement a precautionary measure by using the inverter's communication retry function or communication check function. Refer to your External Device manual for details.
- Do not reset the inverter while communication is enabled. This may cause malfunction. Prior to resetting the inverter, take the Display offline.

## Connection Configuration

- 1:1 Connection

- 1:n Connection

NOTE

- Maximum number of External Devices is 31.

NOTE

- Maximum number of External Devices is 62.

## Communication Settings

Examples of communication settings of the Display and the External Device, recommended by Pro-face, are shown.

WARNING

UNINTENDED EQUIPMENT OPERATION

Read and understand the instructions in this section to ensure data is properly transferred.

## Cable Diagram

The following cable diagrams may be different from cable diagrams recommended by External Device Manufacturer.

Please be assured there is no operational problem in applying the cable diagram shown in this manual.

- The FG pin of the External Device body must be grounded according to your country's applicable standard. Refer to your External Device manual for details.

- SG and FG are connected inside the Display. When connecting the External Device to SG, design your system to avoid short-circuit loops.

- Connect an isolation unit if the communication is not stable due to noise or other factors.

## Supported Devices

Range of supported device address is shown in the table below. Please note that the actually supported range of the devices varies depending on the External Device to be used. Please check the actual range in the manual of your External Device.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Do not simultaneously write to the same register from Display and External Device program.
- Do not write 16-bit word values to registers being accessed in a bitwise manner.

IMPORTANT:

- As shown in the following table, you may need to enter "9999" (meaning an invalid parameter setting or the like) depending upon the parameter types. In this case, the data written and read from the Display is as follows:

  Inverter Series | Inverter Setting | Written Data | Read Data
  --- | --- | --- | ---
  FR-S500/FR-F500J series | --- | -1 (0xFFFF) | -1 (0xFFFF)
  888 | -16 (0xFFF0) | -16 (0xFFF0)
  Series other than above | 9999 | -1 (0xFFFF) | -1 (0xFFFF)
  8888 | -16 (0xFFF0) | -16 (0xFFF0)

### Setting Items List

Word Address | FR-A700/FR-A701 series | FR-F700 series | FR-B,B3(A700) series | FR-B,B3(A500) series
--- | --- | --- | --- | ---
S00 | Operation mode | Operation mode | Operation mode | Operation mode
S01 | Output frequency/speed | Output frequency/speed | Output frequency/speed | Output frequency[speed]
S02 | Output current | Output current | Output current | Output current
S03 | Output voltage | Output voltage | Output voltage | Output voltage
S04 | Special monitor | Special monitor | Special monitor | Special monitor
S05 | Special monitor selection No. | Special monitor selection No. | Special monitor selection No. | Special monitor selection No.
S06 | Output frequency | Output frequency | Output frequency | Output frequency
S07 | Output current | Output current | Output current | Output current
S08 | Output voltage | Output voltage | Output voltage | Output voltage
S09 | Frequency setting | Frequency setting | Frequency setting | Frequency setting
S10 | Running speed | Running speed | Running speed | Running speed
S11 | Motor torque | - | Motor torque | Motor torque
S12 | Converter output voltage | Converter output voltage | Converter output voltage | -
S13 | Regenerative brake duty | Regenerative brake duty | Regenerative brake duty | Regenerative brake
S14 | Electronic thermal relay function load factor | Electronic thermal relay function load factor | Electronic thermal relay function load factor | Electronic overcurrent protection load factor
S15 | Output current peak value | Output current peak value | Output current peak value | Output current peak value
S16 | Converter output voltage peak value | Converter output voltage peak value | Converter output voltage peak value | Converter output voltage peak value
S17 | Input power | Input power | Input power | Input power
S18 | Output power | Output power | Output power | Output power
S19 | Input terminal status | Input terminal status | Input terminal status | -
S20 | Output terminal status | Output terminal status | Output terminal status | -
S21 | Load meter | Load meter | Load meter | -
S22 | Motor excitation current | - | Motor excitation current | -
S23 | Position pulse | - | Position pulse | -
S24 | Cumulative energization time | Cumulative energization time | Cumulative energization time | -
S25 | Orientation status | - | Orientation status | -
S26 | Actual operation time | Actual operation time | Actual operation time | -
S27 | Motor load factor | Motor load factor | Motor load factor | -
S28 | Cumulative power | Cumulative power | Cumulative power | -
S29 | Torque command | - | - | -
S30 | Torque current command | - | - | -
S31 | Motor output | - | Motor output | -
S32 | Feedback pulse | - | - | -
S33 | Power saving effect | Power saving effect | Power saving effect | -
S34 | Cumulative saving power | Cumulative saving power | Cumulative saving power | -
S35 | PID set point | PID set point | PID set point | -
S36 | PID measured value | PID measured value | PID measured value | -
S37 | PID deviation value | PID deviation value | PID deviation value | -
S38 | Option input terminal status1 | - | Option input terminal status1 | -
S39 | Option input terminal status2 | - | Option input terminal status2 | -
S40 | Option output terminal status | - | Option output terminal status | -
S41 | - | - | - | -
S42 | - | - | - | -
S43 | Alarm definition (Latest Nos. 1&2) | Alarm definition (Latest Nos. 1&2) | Alarm definition (Latest Nos. 1&2) | Alarm definition (Latest Nos. 1&2)
S44 | Alarm definition (Latest Nos. 3&4) | Alarm definition (Latest Nos. 3&4) | Alarm definition (Latest Nos. 3&4) | Alarm definition (Latest Nos. 3&4)
S45 | Alarm definition (Latest Nos. 5&6) | Alarm definition (Latest Nos. 5&6) | Alarm definition (Latest Nos. 5&6) | Alarm definition (Latest Nos. 5&6)
S46 | Alarm definition (Latest Nos. 7&8) | Alarm definition (Latest Nos. 7&8) | Alarm definition (Latest Nos. 7&8) | Alarm definition (Latest Nos. 7&8)
S47 | Run command (extended) | Run command (extended) | Run command (extended) | -
S48 | Run command | Run command | Run command | Run command
S49 | Inverter status monitor (extended) | Inverter status monitor (extended) | Inverter status monitor (extended) | -
S50 | Inverter status monitor | Inverter status monitor | Inverter status monitor | Inverter status monitor
S51 | Set frequency read (RAM) | Set frequency read (RAM) | Set frequency read (RAM) | Set frequency read (RAM)
S52 | Set frequency read (EEPROM) | Set frequency read (EEPROM) | Set frequency read (EEPROM) | Set frequency read (EEPROM)
S53 | Set frequency write (RAM) | Set frequency write (RAM) | Set frequency write (RAM) | Set frequency write (RAM)
S54 | Set frequency write (RAM, EEPROM) | Set frequency write (RAM, EEPROM) | Set frequency write (RAM, EEPROM) | Set frequency write (EEPROM)
S55 | Inverter reset | Inverter reset | Inverter reset | Inverter reset
S56 | Alarm definition all clear | Alarm definition all clear | Alarm definition all clear | Alarm definition batch clear
S57 | All parameter clear | All parameter clear | All parameter clear | All clear/User clear
S58 | Link parameter extended setting | Link parameter extended setting | Link parameter extended setting | Link parameter expansion setting
S59 | Second parameter changing | Second parameter changing | Second parameter changing | Second parameter changing

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms