*1

Output frequency/speed

Output frequency[speed]

Output frequency[speed]

Output frequency[speed]

S02

Output current

Output current

Output current

Output current

S03

Output voltage

Output voltage

-

-

S04/SL04*1

Special monitor

-

-

-

S05

Special monitor selection No.

-

-

-

S06/SL06*1

Output frequency

-

-

-

S07

Output current

-

-

-

S08

Output voltage

-

-

-

S09/SL09*1

Frequency setting

-

-

-

S10

-

-

-

-

S11

Motor torque

-

-

-

S12

Converter output voltage

-

-

-

S13

Regenerative brake duty

-

-

-

S14

Electronic thermal relay function load factor

-

-

-

S15

Output current peak value

-

-

-

S16

Converter output voltage peak value

-

-

-

S17

-

-

-

-

S18

Output power

-

-

-

S19

Input terminal status

-

-

-

S20

Output terminal status

-

-

-

S21

-

-

-

-

S22

-

-

-

-

S23

-

-

-

-

S24

Cumulative energization time

-

-

-

S25

-

-

-

-

S26

Actual operation time

-

-

-

S27

Motor load factor

-

-

-

S28

Cumulative power

-

-

-

S29

-

-

-

-

S30

-

-

-

-

S31

-

-

-

-

S32

-

-

-

-

S33

-

-

-

-

S34

-

-

-

-

S35

PID set point

-

-

-

S36

PID measured value

-

-

-

S37

PID deviation value

-

-

-

S38

Option input terminal status1

-

-

-

S39

Option input terminal status2

-

-

-

S40

Option output terminal status

-

-

-

S41

Motor thermal load factor

-

-

-

S42

Inverter thermal load factor

-

-

-

S43

Alarm definition

(Latest Nos. 1&2)

Alarm definition

(Latest Nos. 1&2)

Alarm definition

(Latest Nos. 1&2)

Alarm definition

(Latest Nos. 1&2)

S44

Alarm definition

(Latest Nos. 3&4)

Alarm definition

(Latest Nos. 3&4)

Alarm definition

(Latest Nos. 3&4)

Alarm definition

(Latest Nos. 3&4)

S45

Alarm definition

(Latest Nos. 5&6)

Alarm definition

(Latest Nos. 5&6)

-

-

S46

Alarm definition

(Latest Nos. 7&8)

Alarm definition

(Latest Nos. 7&8)

-

-

S47

Run command (extended)

-

-

-

S48

Run command

Run command

Run command

Run command

S49

Inverter status monitor (extended)

-

-

-

S50

Inverter status monitor

Inverter status monitor

Inverter status monitor

Inverter status monitor

S51/SL51*1

Set frequency read (RAM)

Set frequency read (RAM)

Set frequency read (RAM)

Set frequency read (RAM)

S52/SL52*1

Set frequency read (EEPROM)

Set frequency read (EEPROM)

Set frequency read (EEPROM)

Set frequency read (EEPROM)

S53/SL53*1

Set frequency write (RAM)

Set frequency write (RAM)

Set frequency write (RAM)

Set frequency write (RAM)

S54/SL54*1

Set frequency write

(RAM, EEPROM)

Set frequency write (EEPROM)

Set frequency write (RAM,EEPROM)

Set frequency write (RAM,EEPROM)

S55

Inverter reset

Inverter reset

Inverter reset

Inverter reset

S56

Alarm definition all clear

Alarm definition batch clear

Alarm definition batch clear

Alarm definition batch clear

S57

All parameter clear

All parameter clear

All parameter clear

All parameter clear

S58

Link parameter extended setting

Link parameter expansion setting

Link parameter expansion setting

Link parameter expansion setting

S59

Second parameter changing

Second parameter changing

Second parameter changing

Second parameter changing

*1Available device differs depending on the settings of the External Device. Use the S device and the SL device for 4-byte data length and 6-byte data length, respectively. For details concerning the settings of the External Device, refer to the External Device manual.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms