### Settings of External Device

Use the ladder software for communication settings. (Check the operation in CIMPLICITY Machine Edition V4.50)

1. Select "Add Target" -> "GE Fanuc PLC" among "Project" of tool bar and select the series to be connected.
   The selected series is added as "Target" in the project.

2. Allocate the power supply module and the CPU module in "Hardware Configuration" -> "Main Rack" of added Target.

   NOTE

   - The Rack number and Slot number to allocate by environment using are different.
     Check the environment, and allocate the Rack number and Slot number.

3. Double-click the CPU module, display the setting window.

4. Set the communication settings.

5. Forward the communication settings to the External Device and spend a power supply of the External Device again.

##### Setup Items

[Port1 (RS-485)] tab

Setup Items | Setup Description
--- | ---
Port Mode | SNP
Port Type | Slave
Data Rate [bps] | 19200
Parity | Odd
Stop Bits | 1
SNP ID | 1

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.