Display (Connection Port) | Cable | Note
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT IPC*1 | 7A | Schneider Electric XBTZG919 + Schneider Electric XBTZ9711 (3m) |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

*1Only the COM port which can communicate by RS-232C can be used.