Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 3G | User-created cable + Accessory box by Schneider Electric Industries TSX SCA 50 | Cable length: 10m or less.*3
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) ST6000 2nd Gen*d-4 *d-5 (COM2) PFXST6200AWADI*d-4 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 3I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable + Accessory box by Schneider Electric Industries TSX SCA 50 | Cable length: 10m or less.*3
3A | COM Port Conversion Adapter by Pro-face CA3-ADPCOM-01 + Terminal Block Conversion Adapter by Pro-face CA3-ADPTRM-01 + Accessory box by Schneider Electric Industries TSX SCA 50
3B | User-created cable + Accessory box by Schneider Electric Industries TSX SCA 50
PS5000 PS6000 (Optional Interface) PSA6000 *9 | 3K | User-created cable + Accessory box by Schneider Electric Industries TSX SCA 50 | Cable length: 5m or less.*3

*b-3Except ST-6200

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

*d-5Except PFXST6200AWADI

*3Max length between the Display and the "Accessory Box connected to Display". Total cable length between accessory boxes have to be 1000m or less.

*9Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.