### Settings of External Device

Use the ladder software "TwidoSoft" for communication settings.

Select "Hardware" from "TWDLMDA40DUK" in "Application Browser" of "TwidoSoft", and right-click on "Port 1 : Remote Link, 1" to select "Edit Controller Comm Setup...".
Perform the settings in the "Controller Communication Setup" dialog box displayed next.

Setup Items | Setup Description
--- | ---
Protocol | Type | Modbus
Address | 1
Parameters | Baud Rate | 19200
Data Bits | 8
Parity | None
Stop Bits | 1
End of Frame | 10
Response Timeout | 10 x 100msec
Frame Timeout | 4msec

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.
- Use an integer from 1 to 247 to enter the unit ID of the External Device.