### 5H

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (plug) External Device side: Uni-Telway cable | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) |
(3) | PCMCIA card for RS485 by Schneider Electric Industries TSX SCP 114 |

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.