Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT IPC*2 | 1A | Loader connecting cable by Fuji Electric Systems Co., Ltd.*3 |
GP-4115 (COM1) | 1B | User-created cable + Loader connecting cable by Fuji Electric Systems Co., Ltd.*3 |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently. Displays with Limited Support for Control Signals *2Only the COM port which can communicate by RS-232C can be used. IPC COM Port *3The loader connecting cable differs, depending on the series.

Series | Loader connecting cable type
--- | ---
PXH | ZZPPXH1*TK4H4563
PUM | PUMZ*L01

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.