Display (Connection Port) | Cable | Remarks
--- | --- | ---
GP-4116 (COM1) | 3G | Cable by YASKAWA CONTROLS CO., LTD FADHOWA-50 (0.5m) | Cable length: 30m or less
3H | User-created cable
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) ST6000 2nd Gen*d-4 *d-5 (COM2) PFXST6200AWADI*d-4 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 3I | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 + Cable by YASKAWA CONTROLS CO., LTD FADHOWA-50 (0.5m) | Cable length: 30m or less
3J | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 + User-created cable
3A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + Cable by YASKAWA CONTROLS CO., LTD FADHOWA-50 (0.5m)
3B | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
3C | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 3K | User-created cable | Cable length: 30m or less

*c-2Except ST-6200 *d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently. Displays with Limited Support for Control Signals *d-5Except PFXST6200AWADI *8Only the COM port which can communicate by RS-422/485 (4wire) can be used. IPC COM Port

NOTE

- Maximum cable length is 30m, however, communication may not be possible even when the cable length is less than 30m depending on the use environment. Verify the cable communicates correctly before use.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.