### FX3U, FX3UC-32MT-LT(-2)

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Input Relay | X000 - X377 | X0000 - X0360 |  | *1 *2 *3
Output Relay | Y000 - Y377 | Y0000 - Y0360 | *2
Internal Relay | M0000 - M7679 | M0000 - M7664 |
Special Auxiliary Relay | M8000 - M8511 | M8000 - M8496 | *4
State | S0000 - S4095 | S0000 - S4080 |
Timer (Contact) | TS000 - TS511 | ------ |
Counter (Contact) | CS000 -CS255 | ------ |
Timer (Current Value) | ------ | TN000 - TN511 |
Counter (Current Value) | ------ | CN000 - CN199 |
Counter (Current Value) | ------ | CN200 - CN255 | *5
Data Register | ------ | D0000 -D7999 | *6
Special Data Register | ------ | D8000 - D8511 | *4
Extension Register | ------ | R00000 - R32767 | *4

*1Includes an area in which you cannot write.

*2Specify word address only for the divisible value by 20oct. (Example: X0, X20, X40..., X360)

*3Writing cannot be made to the address, where Input Terminals are allocated on External Device, from Display.

*4Special area. This area may be used by the system, and includes an area in which you cannot write. Please refer to the manual attached to the External Device for more detail.

*532-bit device.

*6You cannot use the data register D7999 as the 32-bit address device. This is because D8000 which is HIGH of the 32-bit device is handled as a different device.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms