### Setting of External Device

Communication settings are made with the ladder software (PCwin). For details on the settings, refer to the Device/PLC Manual.

1. Start the ladder software to start a project.

2. "PC10 Standard" is specified for [CPU Mode] in the project tree.

3. Double-click [Link Parameter] in the project tree.

4. Select the Link No. that you specify the link module in the [Link parameter setup] dialog box, and click [Link setup].

5. Select a link module you use from [Link module name], and click [OK].

   NOTE

   - "Ethernet (32 ports)" can be specified only when the CPU version is V.3.00 or later.

6. Click [Detail] with the specified link module selected and make the settings as shown below.

   Setup Items | Setup Description
   --- | ---
   Own Node IP Address | 192.168.0.1
   Connection 1 | Used
   Open Protocol | TCP Destination-Specified Passive Open
   Own Node Port No. | 1025
   Other Node Table No. | 1
   Initialize | Initialization based on Link Parameter

7. Click [Other Node Table] and make the settings as shown below.

   Setup Items | Setup Description
   --- | ---
   Table 1 | Used
   Other Node IP Address | 192.168.0.2
   Other Node Port No. | 1025

8. Write the communication settings in the External Device. After the writing is completed, restart the External Device.