### 10G)

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: Terminal block | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 |
(3) | Connector conversion cable by Mitsubishi Electric Corp. FX-20P-CADP (0.3m) |

NOTE

- Cable length: 600m or less.