Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT IPC*2 | 9A | RS232C cable by Pro-face CA3-CBL232/5M-01 (5m) + RS422/232C conversion adapter by Panasonic Industrial Devices SUNX Co., Ltd. AFP8550 + Programming cable by Panasonic Industrial Devices SUNX Co., Ltd. AFP1523 (3m) or AFP15205 (0.5m) |
GP-4115 (COM1) | 9B | User-created cable + RS422/232C conversion adapter by Panasonic Industrial Devices SUNX Co., Ltd. AFP8550 + Programming cable by Panasonic Industrial Devices SUNX Co., Ltd. AFP1523 (3m) or AFP15205 (0.5m) |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently. Displays with Limited Support for Control Signals *2Only the COM port which can communicate by RS-232C can be used. IPC COM Port