### Setting of External Device

Use the switches on the side of Ethernet module for setting the External Device.

##### IP Address Setting Switch

Use 8 Hex rotary switches for setting.

Setup Items | Setup Description
--- | ---
IP Address Setting Rotary Switch | Option

##### Port No.

Setup Items | Setup Description
--- | ---
Port No. | 12289 / 12291

##### Condition Setting Switch

DIP Switch | Settings | Setup Description
--- | --- | ---
SW1 | *2 | Data Code
SW2 | OFF | Not protect
SW3 | --- | (Reserved)
SW4 | --- | (Reserved)
SW5 | --- | (Reserved)
SW6 | --- | (Reserved)
SW7*1 | OFF | Close
SW8 | OFF | Normal

*1 SW7 is available to set when the Port No. is 12291.

*2 Set the Data Code in SW1. The setting depends on the Port No.

Port No. | Data Code
--- | ---
ASCII | Binary
12289 | OFF | ON
12291 | ON | OFF

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.