### Settings of External Device

Communication setting of communication module 218IF-01 by ladder software. (Check the operation in MPE720 Ver.5.32)

##### Ladder Software Setting

1. Start ladder software, make an order folder and a PLC folder in a root folder.
   Select the connected PLC at the time of PLC folder making.

2. Click the right button of the PLC which select logon in the displayed menu.

   NOTE

   - Logon after confirming that a check does not begin [online] of a displayed menu.
   - Refer to User's Manual of the PLC about a method of logon.

3. Double-click the [Definition folder]-[Module constitution] of the PLC folder, and display [Engineering Manager].

4. Select the rack classification and link I/F, the pull-down menu in [Controller] of [Engineering Manager].
   Set the number corresponding to the slot number that a communication module uses.
   Select the communication module, setting contents are displayed to [Module details] of [Engineering Manager].

5. Double-click the number part at No. in [Module details].
   Double-click the slot number connecting the ethernet unit.

   Setup Items | Setup Description
   --- | ---
   Transmission parameter | This Station IP address | PLC IP address
   Connection parameter | My Port | PLC port No.
   DST. IP Address*1 | Display IP address
   DST. Port*1 | Display port No.
   Connection type | TCP
   Protocol type | expansion memobus
   Code | BIN

   *1When you check the [Auto] of a port number in the communication setting of the BLUE, set the IP address and the port number to "0.0.0.0" and "00000", respectively.

6. Double-click the "No.1", and set serial communication.
   Use serial communication setting to forward communication setting and the ladder program to the PLC.

7. Save setting content and finish [Engineering Manager].

8. Make the communication ladder "high speed drawing" where "6" is set for [Dev-Typ].

   "Ladder Program for Communication"

9. Turn the DIP switch "INIT" of a communication module to ON, and supply the power.

10. Forward communication setting and a ladder program to a communication module.

11. Log on the PLC in online and write the transferred data to the flash memory.

12. Turn the PLC power and the INIT DIP switch to OFF. Then, turn the PLC power to ON.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.
- Please refer to the manual of the ladder software for more detail.

##### Ladder Program for Communication