Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT IPC*2 | 2A | Cable by Schneider Electric Industries TSX PCX 1031 (2.5m)*3 |
GP-4115 (COM1) | 2B | User-created Cable + Cable by Schneider Electric Industries TSX PCX 1031 (2.5m)*3 |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

*3Set the rotary switch to "3 (OTHER DIRECT)".