### KV-8000 Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | R000000 - R199915 | R0000 - R1999 |  | *6
Output Relay | *6
Internal Auxiliary Relay | *6
Link Relay | B0000 - B7FFF | B000 - B7FF | *5
Internal Auxiliary Relay | MR000000 - MR399915 | MR0000 - MR3999 | *4
Latch Relay | LR00000 - LR99915 | LR000 - LR999 |
Control Relay | CR0000 - CR7915 | CR00 - CR79 |
Work Relay | VB0000 - VBF9FF | VB000 - VBF9F | *5
Timer (Contact) | T0000 - T3999 | ----- | - |
Counter (Contact) | C0000 - C3999 | ----- |
Timer (Setting Value) | ----- | TS0000 - TS3999 |  | *1
Counter (Setting Value) | ----- | CS0000 - CS3999 | *1
Timer (Current Value) | ----- | TC0000 - TC3999 | *1
Counter (Current Value) | ----- | CC0000 - CC3999 | *1
Data Memory | ----- | DM00000 - DM65534 |
Extension Data Memory | ----- | EM00000 - EM65534 |
File Register | Current Bank | ----- | FM00000 - FM32767 |
Serial Number System | ----- | ZF000000 - ZF524287 |
Temporary Data Memory | ----- | TM000 - TM511 |
Control Memory | ----- | CM0000 - CM7599 |
Link Register | ----- | W0000 - W7FFF |
Work Memory | ----- | VM000000 - VM589823 |
Index Register | ----- | Z01 - Z12 | *1 *2
Digital Trimmer | ----- | TRM0 - TRM7 | *1 *3

*132-bit device

*2Z11 and Z12, used by the External Device system, are not available to write in.

*3Write disable.

*4When using KV-EP21V, KV-LE21V or KV-LE20V, the bit addresses are MR00000 - MR99915 and word addresses are MR000 - MR999.

*5The word address descriptions used in the BLUE and the External Device are different. Please be aware of these differences when setting up word addresses.

BLUE | External Device
B000 - B7FF | B0000 - B7FF0
VB000 - VBF9F | VB0000 - VBF9F0

*6When using KV-EP21V, KV-LE21V or KV-LE20V, the bit addresses are R00000 - R99915 and word addresses are R000 - R999.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms