### Setting of External Device

Communication setting of External Device by ladder software (KGL_WIN).

Please refer to the manual of External Device for more detail.

##### Procedure

1. Connect RS-232C port on CPU unit of External Device with the personal computer.
   Turn ON the [BUILT_IN CNET] switch.
   Refer to the manual of External Device for the cable used.

2. Start the ladder software, and make the project newly.
   Select "80S" from [MK_S] of [PLC Type].

3. Double-click [Parameter] of the tree view and display the [Parameter] dialog box.

4. Click the [Comm] tab, and set the communication setup of External Device.

Setup Items | Setup Description
--- | ---
Communication | Enable
Communication Method | Station Number | 0
Baud Rate | 38400
Data Bit | 8
Parity | None
Stop Bit | 1
Communication Channel | RS232C Null Modem or RS422/485
Protocol and Mode | Dedicated | Slave

5. Select [Connect] of the [Online] menu.

6. Select [Write[KGL_WIN=>PLC]] of the [Online] menu, and download the communication setup of External Device.

NOTE

- When [Write[KGL_WIN=>PLC]] cannot be selected, it is necessary to stop driving External Device.
  Select [Change Mode] - [Stop] of the [Online] menu.