### Cable Diagram 1

Display (Connection Port) | Cable | Notes
--- | --- | ---
ST6000 (USB Type-A) ST6000 2nd Gen (USB Type-A) STM6000 (USB Type-A) | 1A | User created cable*1 or Commercially available USB Type-A or USB Type-C communication cable (with ferrite core and shield)*2 | The cable length must be 5m maximum.

*1When creating your own communication cable, ensure the wiring complies with USB 2.0 specifications.
Connect the shield wire to GND to prevent ground loops, and connect only the Display side to the chassis ground.

Signal Name | Type-A Pin No. | Type-C Pin No. | Notes
--- | --- | --- | ---
VBUS | 1 | A4/B4 | +5V Power Supply
D- | 2 | A7/B7 | Data -
D+ | 3 | A6/B6 | Data +
GND | 4 | A1/B1 | Ground

*2Charging-only cables cannot be used. Please prepare a cable that supports data communication.