### Setting of External Device

Use Shenzhen Inovance technology’s setting tool (AutoShop) and rotary switches to configure communication settings on the External Device.

Refer to your External Device manual for details.

##### Setting Tool Setup

1. Start up the setting tool.

2. In [Project Manager], from [Communication Config] double-click [Ethernet].

3. Set the [IP Address] as follows.

   Setting Items | Setting Value
   --- | ---
   IP | 192.168.0
   Subnet | 255.255.255.0

4. Click [OK].

##### Set up CPU

Use rotary switches to set the fourth octet of the IP address.

Rotary switch | Setting Value | Description
--- | --- | ---
1 (x16) | 0 | The fourth octet: 1
0 (x1) | 1

NOTE

- Check with a network administrator about IP address.
  Do not set the duplicate IP address.