*****************************   GP-Pro EX  ****************************
							June 2017
	                                                Pro-face Europe


"Graphical CANopen configuration tool" installer for GP-Pro EX.


Installation: 
=============================
1. Please confirm that the supported software is installed in your computer. 
    Prior to installing, close all your personal computer applications, 
    including any resident programs such as virus detection program, etc

2. After the download to your PC is finished, please extract the zipped archive.

3. Please double-click on IOCAN.exe's icon to start the installer program 

4. After the installer starts, follow the instructions given on each screen

5. After installation, execute GP-Pro EX.

Update History :
==================
V1.3.5.6 (GP-Pro EX 3.5 or later)
V1.3.3.6 (Before GP-Pro EX 3.5)
	[09 Jun. 2017]
	- SP5000 series are now supported. (Requires GP-Pro EX 4.08 or later)
	- Bug fix for modular EDS files with empty module comment fields.
	  (Modules with empty module comments were ignored in the module structure dialog.)
	- Bug fix for HTB configuration dialog. (For RVFC, texts "I3" and "I2" were mistakenly reversed.)

V1.3.4.5 (GP-Pro EX 3.5 or later)
V1.3.3.5 (Before GP-Pro EX 3.5)
	[09 Jan. 2015]
	- Bug fix for LT4000 series.
	When a LT4000 rear module has been selected, GP-Pro EX could show a wrong driver ID in I/O window.

V1.3.4.4 (GP-Pro EX 3.5 or later)
V1.3.3.4 (Before GP-Pro EX 3.5)
	[17 Nov. 2014]
	- Bug fix for EDS with compact storage objects.
	If "CompactSubObj" objects are mapped to PDO in EDS, it could cause an error (error code 13) during startup.

V1.3.4.3 (GP-Pro EX 3.5 or later)
V1.3.3.3 (Before GP-Pro EX 3.5)
	[16 Apr. 2014]
	- Bug fix for modular objects.
		When both FixedObject and SubExtObject define the same object, the device catalog could get corrupted
		and the CANopen configuration editor did not function anymore.

V1.3.4 (GP-Pro EX 3.5 or later)
V1.3.3 (Before GP-Pro EX 3.5)
	[30 Aug. 2013]
	This version requires GP-Pro EX version 3.5 or higher.
	The following feature has been added
	- LT4000 CANopen master configuration support
	
V1.3.3
	[01 Jun. 2012]
	This version (and older) requires GP-Pro EX versions older than 3.5.
	The following issue has been corrected
	- Wrong captions for RVFC0 auxiliary inputs
	- Abrupt termination when using a slave with T/R PDO 256-511
	
V1.3.2
	[11 Jan. 2012]
	The following issue has been corrected
	- The dialog crashes in HTB analog module configuration.
	- Missing buttons under Japanese Windows operation systems.
        The following features are added
	- An extra warning message when setting 0 to HTB counter preset value.
	- Installer supports GP-Pro EX 3.0

V1.3.1
	[01 Sep. 2010]
	Newly released
	
No part of this document may be used or reproduced without permission.
****************************  End of Readme  *****************************
