Install the chipset drives for 82801DB and 82845G chipset before installing any
other drivers.

To install the driver, save any unsaved work and close all applications, then click on
the .exe file to begin extracting the files.
Finally, follow the prompts and restart at the end of the installation.

To enable the touchscreen, double click on the desktop icon then press the [ENTER] key
when the prompt for going to the next screen appears. When the calibation screen appears
select "Add" to search for and add the touch controller (It should show up on COM3).
Next, select "Advanced" and do a 25 point calibration. If you're satisfied with the
calibation save a exit.

