Xycom self extracting zip file for XP/2000 serial/USB combo driver is 5015_R2_w2k_xp.exe.

Windows XP/2000 Universal
Download Version Windows OS Interface  Technology  Notes 
sw500930.exe - Xycom name 5015_R2_w2k_xp.exe
(2.4 MB) 4.30 XP, 2000  USB, Serial  All  
Windows Hardware Quality Lab (WHQL) certified for serial and USB interface. This driver supports multiple
monitors but does not support full-screen DOS applications. An HTML user's manual is included in this
download; it is also separately available under Installation Notes. 


Xycom self extracting zip file for both 98 serial and USB driver is 5015_R2_win98.exe. It contains:

Windows 98/98SE/Me USB
Download Version Windows OS Interface  Technology  Notes 
sw500917.exe - Xycom name 98_ME_USB.exe
(277K) 1.00c Me, 98SE, 98  USB  All  This driver does not support full-screen DOS applications.

Windows 95/98/98SE/Me Serial
Download Version Windows OS Interface  Technology  Notes 
sw500085.exe - Xycom name 98_ME_Ser.exe
(354K)  3.01 Me, 98SE, 98, 95  Serial  All  Supports up to 4 monitors. To use touchscreens with DOS applications on this operating system, you must use the Win 3.1/DOS drivers, not this driver.
 

Xycom self extracting zip file for the NT4.0 serial driver is 5015_R2_nt4.exe.

Windows NT Serial
Download Version Windows OS Interface  Technology  Notes 
sw000107.exe - Xycom name 5015_R2_nt4.exe
(269K)  4.0 NT  Serial  All  For Win NT 4.0; version 4.0 with updated User Interface for Single Monitor applications. For multiple monitor applications, use version 3.10C.
