Copyright (c) By Salt International Corp. All rights reserved. 
  
PENMOUNT WINDOWS 98/ME DRIVER FOR DMC9000 INSTALLATION
This driver supports Windows 98/ME system. The detailed contents of PenMount Windows 98/ME driver for DMC9000 is list below:
OS.DAT
_ISDEL.EXE
SETUP.EXE
LANG.DAT
_INST32I.EX_
_SETUP.DLL
SETUP.INS
_SYS1.CAB
SETUP.BMP
DATA.TAG
SETUP.INI
_USER1.CAB
CONFIG.INI
DATA1.CAB
README.TXT
LAYOUT.BIN
SETUP.LID

There are several functions in PenMount Windows 98/ME drivers: 

1. PenMount monitor : After PenMount Windows 98/Me driver installed, the PenMount monitor will appear on the menu bar of the system. It is easy for user to call other PenMount utilities or functions on line.

2. Supporting Plug and Play: After installing PenMount Windows 98/Me drivers, the system automatically detects the COM port that touch screen connected to. 

3. Beep sound on/off

4. Right button selectable: This emulates mouse right button function on touching.

5. Drawing test.

6. Uninstall utilities: Use this to remove PenMount Windows 98 driver from system


PenMount Windows 98/ME Driver Installation

To install the software to your computer, you must have Windows 98 (or Windows ME) system running and a PenMount Windows 98/ME driver . If you have an older version PenMount Windows 98/ME driver installed in your system, please remove it first. 

Follow the steps below to install the PenMount Windows 98/ME driver.  

Insert PenMount Windows 98/ME driver to your computer. From the "Start" menu, select "Run". There is one entry "setup.exe" in PenMount Windows 98/ME driver.  Use browse to find it or type in "X:\setup.exe" to execute it.

The screen displays PenMount Logo and "PenMount Utilities Setup", and then show 'PenMount Utilities for Win98/ME" screen plus "welcome" message appears. Select "Next".

The next screens are "Software License Agreement" and "Information", select "Yes" and "Next'.

The next screen is "Choose Destination Location". It is for Setup installing PenMount Utilities in the folder: C:\Program Files\PenMount\Win9X, select "Next' or modify the folder name you like to use.

The next screen is "Select Program Folder, the default is set at "PenMount Utilities", select "Next' or change it.

The screen is showing "Start Copying Files", select "Next" for starting copy files to system.

The screen now is "Setup Complete", select "Finish". Now, the system will ask you to reboot the computer. After rebooting the touch panel can work well. 

The 'PenMount Utilities' now is in the 'Programs', you could have the 'PenMount Monitor' appeared in the menu bar for easily selecting PenMount funcitons.

We suggest you do "Calibrate" now to adjust the screen and touch cursor matched properly, from 'PenMount Utilities', select 'Calibrate' from "PenMount Control Panel".

Function Description:
--- "PenMount Control Panel": This is at PenMount "Utilities" of "Programs". There are following functions on it:


- Calibrate: click it and follow the instructions to do calibration by touching mid-top, mid-right, mid-bottom and mid-left.  After calibration done, it is suggested to go to Draw to test the result.

- Draw: Test or demonstrate PenMount touch screen operation

- About: PenMount information

--- PenMount Monitor: there are following utilities on it, "Right Click Button", "Beep Sound" and "Exit". These are for user easily use PenMount utilities.

--- Uninstall: this utility is for removing PenMount Windows 98/ME driver V2.1 from system. If your PenMount Windows 98/ME is a previous version, please see Q&A for how to remove it.

--- ReadMe: this file.


Salt International Corp.
Dec. 2001

Question and Answer:
Q1: What is the update version of PenMount Windows 98 and Windows ME driver?
A1: The updated version is V2.1

Q2: Can PenMount Windows 98 driver support Windows 95 system?
A2: Please use V2.0 for Windows 95 system.

Q3: How can I uninstall the PenMounut Windows 98/ME V2.1 driver.
A3: Before you uninstall PenMount Windows 98/Me driver, please ¡¥EXIT¡¦ the ¡¥PenMount monitor¡¦ in menu bar first.
    From PenMount Utilities¡¦of Programs¡¦,select Uninstall¡¦utility, computer will ask you are you sure you want to completely remove PenMount Utilities¡¦and all its components¡¨? Select ¡¥Yes¡¦ to remove PenMount Windows 98/Me driver.


