# Intel® PRO/Wireless LAN Products
Safety and Regulatory Notices

This document contains regulatory notices for the following products:

- Intel® PRO/Wireless 5000 LAN Products
- Intel® PRO/Wireless 2011B LAN Products

## Intel® PRO/Wireless 5000 LAN Products

This section provides the following safety and regulatory notices covering the following products: Intel® PRO/Wireless 5000 LAN Access Point and Intel® PRO/Wireless 5000 LAN CardBus Adapter.

### Safety Notices

The FCC with its action in ET Docket 96-8 has adopted a safety standard for human exposure to radio frequency (RF) electromagnetic energy emitted by FCC certified equipment. The Intel PRO/Wireless 5000 LAN products meet the Human Exposure limits found in OET Bulletin 65, 2001, and ANSI/IEEE C95.1, 1992. Proper operation of this radio according to the instructions found in this manual will result in exposure substantially below the FCC’s recommended limits.

- Do not touch or move antenna while the unit is transmitting or receiving.
- Do not hold any component containing the radio such that the antenna is very close or touching any exposed parts of the body, especially the face or eyes, while transmitting.
- Do not operate the radio or attempt to transmit data unless the antenna is connected; if not, the radio may be damaged.
- Use in specific environments:
  - The use of wireless devices in hazardous locations is limited by the constraints posed by the safety directors of such environments.
  - The use of wireless devices on airplanes is governed by the Federal Aviation Administration (FAA).
  - The use of wireless devices in hospitals is restricted to the limits set forth by each hospital.
- Antenna use:
  - In order to comply with FCC RF exposure limits, low gain integrated antennas should be located at a minimum distance of 7.9 inches (20 cm) or more from the body of all persons.
  - High-gain, wall-mount, or mast-mount antennas are designed to be professionally installed and should be located at a minimum distance of 12 inches (30 cm) or more from the body of all persons. Please contact your professional installer, VAR, or antenna manufacturer for proper installation requirements.
- Explosive Device Proximity Warning (see below)
- Antenna Warning (see below)
- Use on Aircraft Caution (see below)
- Other Wireless Devices (see below)
- Power Supply (Access Point) (see below)

#### Explosive Device Proximity Warning

Warning: Do not operate a portable transmitter (such as a wireless network device) near unshielded blasting caps or in an explosive environment unless the device has been modified to be qualified for such use.

#### Antenna Warning

Warning: To comply with the FCC and ANSI C95.1 RF exposure limits, it is recommended when using a wireless device with an integrated antenna (whether an Access Point, a PC Card inserted into a laptop computer, or a PCI or MiniPCI card installed in a desktop computer), that the antenna should not be positioned closer than 5 cm (two inches) from your body or 6ther persons for extended periods of time while it is transmitting (or operating). If the antenna is positioned less than 5 cm (two inches) from the user, it is recommended that the user limit exposure time.

#### Use On Aircraft Caution

Caution: Regulations of the FCC and FAA prohibit airborne operation of radio-frequency wireless devices because their signals could interfere with critical aircraft instruments.

#### Other Wireless Devices

Safety Notices for Other Devices in the Wireless Network: Refer to the documentation supplied with wireless Ethernet adapters or other devices in the wireless network.

#### Power Supply (Access Point)

Use manufacturer-provided power supply with output rating 5.0 VDC and 2.5 A.

### FCC Regulations

#### FCC Regulations Part 15 Declaration of Conformity (DoC)

Intel Corporation declares that the equipment described in this document is within the requirements of the Code of Federal Regulations listed below:

Title 47 Part 15, Subpart B, Class B for a digital device.

This declaration is based upon the compliance of the Intel® PRO/Wireless 5000 LAN Access Point model WSAP5000, the Intel PRO/Wireless CardBus Adapter model WCB5000, and the Intel PRO/Wireless PCI Adapter model WPCI5000 to the above standards. Intel has determined that the models listed have been shown to comply with the applicable technical standards if no unauthorized change is made in the equipment and if the equipment is properly maintained and operated.

These units are identical to the units tested and found acceptable with the applicable standards. Records maintained by Intel continue to reflect that units being produced under this Declaration of Conformity, within the variation that can be expected due to quantity production and tested on a statistical basis, continue to comply with the applicable technical standards.

#### FCC Rules and Regulations - Part 15

This device complies with Part 15 of the FCC rules. Operation is subject to the following two conditions:

1. This device may not cause harmful interference and,
2. This device must accept any interference received, including interference that may cause undesired operation.

This equipment has been tested and found to comply with the limits for a Class B digital device pursuant to Part 15 of the FCC rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation. This equipment generates, uses, and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation. If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

- Reorient or relocate the receiving antenna.
- Increase the separation between the equipment and the receiver.
- Connect the equipment into an outlet on a circuit different from that to which the receiver is connected.
- Consult the dealer or an experienced radio/TV technician for help.

CAUTION: The Part 15 radio device operates on a non-interference basis with other devices operating at this frequency. Any changes or modification to said product not expressly approved by Intel could void the user's authority to operate this device.

### Canadian Department of Communications Industry Canada (IC) Notice

These digital apparatuses do not exceed the Class B limits for radio noise emissions from digital apparatuses set out in the Radio Interference Regulations of the Canadian Department of Communications.

Les présents appareils numériques n'ément pas de bruits radioélectriques dépassant les limites applicables aux appareils numériques de Classe B prescrites dans le règlement sur le brouillage radioélectrique édicté par le Ministère des Communications du Canada.

These devices comply with Class B Limits of Industry Canada. Operation is subject to the following two conditions:

1. The device may not cause harmful interference, and
2. The device must accept any interference received, including interference that may cause undesired operation.

These devices are certified to the requirements of ANSI/IEEE C95.1-1992 and RSS-210 for 5 GHz UNII band devices. The use of these devices in a system operating either partially or completely outdoors may require the user to obtain a license for the system according to the Canadian regulations. For further information, contact your local Canada Industry office.

### Japan Regulatory Notices

#### TELEC

This equipment has been certified to conform with the technical regulations of the specified radio equipment under the radio law of Japan. If you open the case to modify the circuit, you may be punished by law.

This equipment is for indoor use only under the Radio Wave law.

### JATE

Refer to the JATE approval number on the equipment.

## Intel® PRO/Wireless 2011B LAN Products

### Radio Frequency Interference Requirements – USA

This device uses, generates and radiates radio frequency energy. The radio frequency energy produced by this device is well below the maximum exposure allowed by the Federal Communications Commission (FCC).

This device complies with the limits for a Class B digital device pursuant to Part 15 subpart C of the FCC Rules and Regulations. Operation is subject to the following two conditions:

1. This device may not cause harmful interference.

2. This device must accept any interference received, including interference that may cause undesired operation.

The FCC limits are designed to provide reasonable protection against harmful interference when the equipment is installed and used in accordance with the instruction manual and operated in a commercial environment. However, there is no guarantee that interference will not occur in a particular commercial installation, or if operated in a residential area.

If harmful interference with radio or television reception occurs when the device is turned on, the user must correct the situation at the user’s own expense. The user is encouraged to try one or more of the following corrective measures:

- Re-orient or relocate the receiving antenna.

- Increase the separation between the equipment and receiver.

- Connect the equipment into an outlet on a circuit different from that on which the receiver is connected.

- Consult the dealer or an experienced radio/TV technician for help.

### Radio Frequency Interference Requirements – Canada

This Class B digital apparatus complies with Canadian ICES-003, Issue 2, and RSS-210, Issue 4 (Dec. 2000).

“To prevent radio interference to the licensed service, this device is intended to be operated indoors and away from windows to provide maximum shielding. Equipment (or its transmit antenna) that is installed outdoors is subject to licensing.”

Cet appareil numérique de la classe B est conforme à la norme NMB-003,

No. 2, et CNR-210, No. 4 (Dec. 2000).

« Pour empêcher que cet appareil cause du brouillage au service faisant l'objet d'une licence, il doit être utilisé à l'intérieur et devrait être placé loin des fenêtres afin de fournir un écran de blindage maximal. Si le matériel (ou son antenne d'émission) est installé à l'extérieur, il doit faire l'objet d'une licence. »

### Radio Frequency Interference Requirements – European Union

#### CE Marking & European Union Compliance

| Products intended for sale within the European Union are marked with the Conformite Europeene (CE) Marking, which indicates compliance with the applicable Directives and European Normes, and amendments, identified below.
| This equipment also carries the Class 2 identifier.

##### English

This product follows the provisions of the European Directive 1999/5/EC.

##### Danish

Dette produkt er i overensstemmelse med det europæiske direktiv 1999/5/EC

##### Dutch

Dit product is in navolging van de bepalingen van Europees Directief 1999/5/EC.

##### Finnish

Tämä tuote noudattaa EU-direktiivin 1999/5/EC määräyksiä.

##### French

Ce produit est conforme aux exigences de la Directive Européenne 1999/5/EC.

##### German

Dieses Produkt entspricht den Bestimmungen der Europäischen Richtlinie 1999/5/EC.

##### Greek

Το προϊόν αυτό πληροί τις προβλέψεις της Ευρωπαϊκής Οδηγιας 1999/5/EC.

##### Icelandic

Þessi vara stenst reglugerð Evrópska Efnahags Bandalagsins númer 1999/5/EC.

##### Italian

Questo prodotto è conforme alla Direttiva Europea 1999/5/EC.

##### Norwegian

Dette produktet er i henhold til bestemmelsene i det europeiske direktivet 1999/5/EC.

##### Portuguese

Este produto cumpre com as normas da Diretiva Européia 1999/5/EC.

##### Spanish

Este producto cumple con las normas del Directivo Europeo 1999/5/EC.

##### Swedish

Denna produkt har tillverkats i enlighet med EG-direktiv 1999/5/EC.

### Applicable Directives

Electromagnetic Compatibility Directive 89/336/EEC

Low Voltage Directive 73/23/EEC

Radio and Telecommunication Terminal Equipment 1999/5/EC

### Applicable Standards

EN 50 082-1 – 1997 Electromagnetic Compatibility – Generic Immunity Standard, Part 1: Residential, Commercial, Light Industry

EN61000-4-2 – Electromagnetic Compatibility for Industrial Process Measurement and Control Equipment, Part 2: Electrostatic Discharge Requirements

EN61000-4-3 – Electromagnetic Compatibility for Industrial Process Measurement and Control Equipment, Part 3: Radiated Electromagnetic Field Requirements

EN61000-4-4 – Electromagnetic Compatibility for Industrial Process Measurement and Control Equipment, Part 4: Electrical Fast Transients Requirements

EN61000-4-5 – Surge Immunity Tests Basic EMC Standard

EN61000-4-6 – Immunity to Conducted Disturbances, Induced by Radio Frequency Fields

EN61000-4-11 – Voltage Dips, Short Interruptions and Voltage Variations

EN 300 328-2 V1.1.1 (2000-07) – Radio Equipment and Systems (RES); Wideband transmission systems; Technical characteristics and test conditions for data transmission equipment operating in the 2.4 GHz ISM band and using spread spectrum modulation techniques

ETS 300 826:1997 – Electromagnetic compatibility and Radio spectrum Matters (ERM); Electromagnetic Compatibility (EMC) standard for

2.4 GHz wideband transmission systems and High Performance Radio Local Area Network (HIPERLAN) equipment. This is a basic standard called out by EN 301 489-17.

EN 301 489-17 v1.1.1 (2000-09) – Electromagnetic Compatibility (EMC) standard for radio equipment and services; Part 17: Specific conditions for Wideband data and HIPERLAN equipment.

EN 55022:1998 – Information technology equipment – Radio disturbance characteristics – Limits and methods of measurement

EN 55024:1998 – Information technology equipment – Immunity characteristics – Limits and methods of measurement

EN 61000-3-2:1995 +A14 – Electromagnetic compatibility (EMC)

Part 3-2: Limits – Limits for harmonic current emissions (equipment input current up to and including 16 A per phase)

EN 61000-3-3:1995 – Electromagnetic compatibility (EMC),

Part 3-3: Limits – Limitation of voltage fluctuations and flicker in low-voltage supply systems for equipment with rated current up to 16 A

EN 60950:1992 + A1 – A4, A11 – Safety of Information Technology Equipment, including Electrical Business Equipment

### European Economic Area Restrictions

The European variant is intended for use throughout the European Economic Area; however, authorization for use is restricted as follows:

European standards dictate maximum radiated transmit power of 100mW EIRP and frequency range 2.400 to 2.4835 GHz.

In France, the equipment must be restricted to the 2.4465 to 2.4835 GHz frequency range and must be restricted to indoor use.

In Belgium when used outside, the equipment must be restricted to the 2.460 to 2.4835 GHz frequency range.

Operation in Italy requires a user license.

In Hungary, Processing gain minimum 10 dB, integral or external antenna with maximum 6 dBi gain.

In the Netherlands, 10 mW indoor and outdoor with no license. 100 mW indoor with no license. 100 mW with license outdoor within 2451 - 2471 MHz.

### Japanese Notices

### RF Devices

Intel Radio Frequency (RF) products are designed to be compliant with the rules and regulations in the locations where they are sold and are locally labeled as required. The majority of Intel RF devices are type-approved and do not require the user to obtain license or authorization before using the equipment. However, any changes or modifications to Intel equipment not expressly approved by Intel could void the user’s authority to operate the equipment.

Caution: Do not attempt to operate this device with a modified or damaged antenna.

Warning: To comply with FCC rules for RF exposure, maintain a minimum separation distance of 20 cm (8 inches) between the Intel® PRO/Wireless 2011B LAN Access Point radiating elements and nearby persons.

[legal.htm]