A B C D E F I L M N P R S T U W

    A

    access point
        how many APs to use
        Intel PRO/Wireless 5000 LAN
        Intel PRO/Wireless 2011B or 2011 LAN
        IP address
        LEDs

    Administration Tools
        AP Discovery
        installation
        site survey
        starting

    AP Discover Utility
        default IP address
        DHCP
        starting

    attenuation

    B

    bridge

    BSSID

    C

    channel selection

    client association

    connecting to an AP

    D

    Direct-Sequence Spread Spectrum

    data encryption

    data rates

    E

    encryption

        description
        Wired Equivalent Privacy (WEP)

    ESSID

    F

    FCC compliance

    frequency interference

    FTP test

    I

    ICMP tests

    infrastructure mode

    interference

    IP address for an access point
    installation

    L

    LEDs

    M

    MAC address

    minimum separation

    N

    network name

    noise Info

    P

    peer-to-peer mode

    R

    repeater

    RF exposure

    RF interference

    S

    security

    selecting adapters

    signal quality

    site size

    site planning

    Site Survey Utility
        creating

        channel selection
        conducting a site survey
             effective site survey
             electrical power
             environmental interference
             equipment and materials
             medium or large area
             performing a site survey
             preparing for an site survey
             size and shape of the site
             small area
        creating a wireless LAN
        Network Name (SSID)
        network usage requirements
        reports

        starting

        using the Site Survey Utility
        when to perform a site survey

    SSID

    T

    topology

    U

UPS
using Site Survey
usage requirements

    W

    WEP
    WLAP Mode
    Windows drivers installation
    wiring to use
    Wired Equivalent Privacy (WEP)
    Wireless LAN networking overview