# Introduction

The 802.11a Intel® PRO/Wireless 5000 LAN Access Point operates in the 5 GHz spectrum at speeds up to 54 Mbps. It features a software configurable antenna and supports IEEE 802.3af Power over Ethernet. Each access point uses eight non-overlapping transmission channels for support of up to 64 active users per access point. Placement can be on a desk or table, mounting on a wall or ceiling.

The PRO/Wireless 5000 LAN Access Point is compatible with other products supporting the IEEE 802.11a standard.

Security features include support for 128, 64, and 0-bit Wired Equivalent Privacy (WEP) encryption and Virtual Private Network (VPN) compatibility.

A browser-based user interface is provided for configuration of the access point. See the installation instructions for information on how to set up and configure one or more access points.

For information on how to set up a wireless LAN, see the Administrator's Guide. This document is intended for use by network administrators.

Copyright © 2002 Intel Corporation. Legal Information