# Intel Network Driver for Caldera* OpenServer*

Instructions for Installing the eeE Driver for Caldera* (formerly SCO*) OpenServer*:

1. Copy the eee.vol file to any directory, such as /tmp. Rename the file as VOL.000.000, and make the file read-only by using 'chmod'. For example:

   > cp eee.vol /tmp/VOL.000.000
   > chmod 444 /tmp/VOL.000.000

2. If there is an older version of the eeE driver on the system, you must first remove it. To do this, run 'netconfig'. Remove all instances of the "Intel ..." adapters. Exit netconfig without opting to relink the kernel. Run 'custom'. Remove the older driver for the Intel adapter.

3. Install the new driver using 'custom'. When asked for the installation media, choose media images, and type the directory path to the VOL.000.000 file. (In step 1, if you copied it to /tmp, type /tmp). After the installation of the driver is complete, exit 'custom'.

4. Run 'netconfig' and add the adapters. For each adapter that is present in the system, enter the appropriate TCP/IP parameters. By default, the driver automatically detects the line speed and duplex mode. If you want to force any of these settings, choose Advanced Options and set the speed and duplex modes. Exit 'netconfig' and choose the option to relink the kernel.

5. Reboot the system.

Copyright © 2002 Intel Corporation. Legal Information