## Configure the Access Control List

The Access Control List (ACL) contains MAC addresses for clients allowed to associate with the access point. This provides security by preventing unauthorized access. The ACL supports adding client computer entries by individual MAC address or by a range of MAC addresses. The maximum number of entries is 512 if no entries have been made for Disallowed Address Filtering. Only 512 entries are available to both ACL and Disallowed Address Filtering.

1. Select the Set Access Control List option from the Main Menu to display:

>      Address Type?   range individual

1. Use the UP/DOWN-ARROW keys to toggle between range and individual .

### Setting a Range of Allowed Clients

To select a range of MAC addresses:

1. Type in the minimum MAC address as the top value:

>      00:0A:F8:F0:01:01

2. Press ENTER to accept the value; use the DOWN-ARROW key to select the maximum value.
3. Type in the maximum MAC address in the bottom value:

>      00:0A:F8:F0:02:FF

1. Press ENTER to accept the value. Use the DOWN-ARROW key to select OK.
2. Press ENTER and change the values as needed.
3. To delete a range of wireless clients, select Delete-[F1].
4. To add a range of wireless clients, select Add-[F2].
5. Select S ave ALL APs-[F3] to save the Ranges of Allowed Mobile Units information to all access points with the same SSID. This option saves the configuration changes for the current access point, and sends two messages to all other access points on the Known APs table to update their configuration and reset after the configuration has been modified. You can perform this option only among the same hardware platforms and firmware versions.

When you enable the Access Control option, all clients within the specified range can associate with the access point. Specify additional ranges as needed or add to the ACL using individual address entries.

### Adding Allowed Clients

The Access Control List screen provides a facility to add clients to the ACL.

1. Select the Set Access Control List option from the Main Menu to display:

>      Address Type? range individual

2. Use the UP/DOWN-ARROW keys to toggle between range and individual. Select individual.
3. Press Add-[F2]. The access point prompts for a MAC address.

>      00:00:00:00:00:00

4. Enter the MAC address. You can enter MAC addresses without colons.
5. Select Save ALL APs-[F3] to save the Access Point Installation configuration information to all access points with the same SSID. This option saves the configuration changes for the current access point, and sends two messages to all other access points on the Known APs table to update their configuration and reset after the configuration has been modified. You can perform this option only among the same hardware platforms and firmware version.

### Removing Allowed Clients

The Allowed Mobile Units screen provides a facility to remove clients from the ACL.

1. Highlight the entry using the UP/DOWN-ARROW keys.
2. Press Delete - [F1].

### Enabling or Disabling the Access Control List

To switch between enable or disable locate the ACL in the System Configuration screen.

1. Select Set System Configuration from the Main Menu .
2. Press TAB to select Access Control .
3. Press SPACE BAR to Enable .
4. Select Save to save changes.

### Removing All Allowed Clients

The access point provides a facility to remove all clients from the ACL.

1. Select Special Functions from the Main Menu .
2. Select Clear ACL .

### Loading an Access Control List from the Computer (MU) List

This option from the Special Functions menu takes all associated clients and creates an ACL from them. This quickly builds an ACL without having to manually type addresses and can be edited using the add and delete functions.

To add addresses of associated clients to the ACL:

1. Select Special Functions from the Main Menu.
2. Select Load ACL from Computer List.

### Loading an Access Control List from File

This option from the Special Functions menu creates an access control list from a user-defined file. The file is entered on the secondary screen of the Special Functions Menu. Follow this link to view an example of the AP_ACL.TXT file.

1. Select Special Functions from the Main Menu .

2. Select Load ACL from File to load site specific ACL.

## Clearing Clients from the Access Point

You can clear the client computer association table for diagnostic purposes. Clear clients from the access point if the access point has many client associations no longer in use. Use this option to make sure that clients associating with the access point are active.

To clear clients associated with the access point:

1. Select Special Functions from the Main Menu .
2. Select Clear MU Table . The access point removes the clients associated with it. Clients cleared from the access point try to reassociate with the access point or another nearby access point.

Copyright © 2002 Intel Corporation. Legal Information