## Interface Statistics

The Interface Statistics screen provides packet forwarding statistics for each interface (Ethernet, RF, AP) and performance information for each interface in packets per second (PPS) and bytes per second (BPS).

The access point interface indicates packets sent to the access point protocol stack (e.g. configuration requests, SNMP, Telnet).

### Web Interface

1. Select Interface from the Statistics Menu at the left side of the screen.
2. Click Start Refresh to update the values on the screen.
3. When finished, click Stop Refresh.

### Console Management

1. Select I nterface Statistics from the Main Menu .
2. Select Refresh at the status display to update the values manually.
3. Select Timed to automatically update this display every two seconds.
4. Press ESC to return to the previous menu

Copyright © 2002 Intel Corporation. Legal Information