# Intel® PRO/Wireless 5000 LAN Products
Specifications

## Specifications by Model
Models | Intel® PRO/Wireless 5000 LAN Access Point model WSAP5000 Intel® PRO/Wireless 5000 LAN CardBus Adapter model WCB5000 Intel® PRO/Wireless 5000 LAN PCI Adapter model WPCI5000
Access Point Physical Specifications | Form Factor | Access Point
Dimensions | 10” x 9.9” x 4.2” (36 cm x 33 cm x 14 cm)
Weight | 4 lb (181 g)
Connector Interface | RJ-45
LEDs | See LED Indicators
Power | 110 Volt AC Adapter
CardBus Adapter Physical Specifications | Form Factor | CardBus Type II Extended
Dimensions | 2.2" x 4.4" x 0.19" (54 mm x 112 mm x 5 mm) 3" (7.8 mm) on extended portion
Weight | 5 oz (29 g)
Connector Interface | 68-pin CardBus
LEDs | Link, Activity
Power | 50 mW
PCI Adapter Physical Specifications | Form Factor | PCI Adapter
Dimensions | 6.6 " x 2.5 (20 cm x 5 cm)
Weight | 5 oz (29 g)
Connector Interface | PCI
LEDs | Link, Activity
Power | 3.3 V
## General Specifications
Frequency and modulation | Frequency band | 5.15 GHz to 5.35 GHz
Modulation | BPSK, QPSK, 16 QAM, 64 QAM
Wireless Medium | Orthogonal Frequency Division Multiplexing (OFDM) 5 GHz UNII
Channels | 8 Non-overlapping
Network | WLAN Standard | IEEE 802.11a
Wired Standard | 10/100BTx
Architecture | Infrastructure, ad-hoc (peer-to-peer)
Roaming | 802.11a compliant for seamless roaming between access points International roaming (802.11d)
Wired-to-wireless switching | Intel® PROSet II software
Security | Encryption | 64-bit and 128-bit WEP
| 802.11i (802.1x, Radius, EAP): enhanced wireless LAN encryption and authentication security | Pending IEEE ratification in 2002
QOS | DCF | CSMA/CA
Range and Throughput | Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps with the following range capabilities:
Indoor Range | 40 feet @ 54 Mbps 300 feet @ 6 Mbps
Outdoor Range | 100 feet @ 54 Mbps 1000 feet @ 6 Mbps
Throughput | Up to 15 Mbps
Power | Output Power | 40 mW to 200 mW, depending on frequency channel
Transmit | 450-480 mA
Receive | 420-440 mA
Idle | <420 mA
Standby | <30 mA
Voltage | 3.3 V
Operating Temperature | 0 to +65 Celsius |
Humidity | 10 to 90% non-condensing |
Compatibility | OS | Microsoft Windows* 98SE*, Me*, 2000*, XP*
WECA | Pending ratification of interoperability test and logo program by WECA (when 5 GHz standard is available)
WHQL | Yes
Regulatory and Safety | Safety | UL, C-UL
United States | FCC
Canada | Industry Canada
Japan | VCCI, JATE, Telec

# Intel® PRO/Wireless 2011B LAN Products
Specifications

## Specifications by Model
Models | Intel® PRO/Wireless 2011B LAN Access Point model xxx Intel® PRO/Wireless 2011B LAN Adapter model xxx
Access Point Physical Specifications | Form Factor | Access Point
Dimensions | 1.75” x 6” x 8.5” (4.4 cm x 15.2 cm x 21.6 cm)
Weight (w/power supply) | 1 lb (454 g)
Connector Interface | RJ-45
LEDs | See LED indicators.
Power | 110 Volt AC Adapter
Adapter Physical Specifications | Form Factor | CardBus Type II, 3.3V
Dimensions | 3.3" x 2.1" x 0.2" (85 mm x 54 mm x 5 mm)
Weight | 1.6 oz (45.4 g)
Connector Interface |
LEDs | See LED indicators.
Power |
## General Specifications
Frequency and modulation | Frequency band | country dependent, typically 2412 MHz to 2462 MHz
Modulation | Binary GFSK
Wireless Medium |
Channels | 3 Non-overlapping
Network | WLAN Standard | IEEE 802.11b
Wired Standard | 10/100B Tx
Architecture | Infrastructure, ad-hoc (peer-to-peer)
Roaming | 802.11b compliant for seamless roaming between access points International roaming (802.11d)
Wired-to-wireless switching | Intel® PROSet II software
Security | Encryption | 64-bit and 128-bit WEP
QOS | DCF |
Range and Throughput | Data Rates | 11 Mbps - Optional 5.5 Mbps - Optional 2 Mbps - Required 1 Mbps - Required
Indoor Range | 30 to 50 feet @ 11 Mbps
Outdoor Range | 100 feet @ 11 Mbps
Throughput | Up to 11 Mbps
Power | Output Power |
Transmit |
Receive |
Idle |
Standby |
Voltage | 3.3 V
Operating Temperature | 0 to 55° Celsius |
Humidity | 10 to 95% non-condensing |
Compatibility | OS | Windows 95C, 98SE, Me, 2000
WECA | Yes
WHQL | Yes
Regulatory and Safety | Safety | UL, C-UL
United States | FCC part 15.247
Canada | Industry Canada
Europe | ETS 300 320
Japan | RCR STD-33

Copyright © 2002 Intel Corporation. Legal Information