## Testing Connection Quality

This feature is useful when two access points, each connected to their own network, communicate with each other. The access points maintain a wireless connection and function as a bridge between the two Ethernet networks. The Link Test feature allows you to determine the best antenna alignment between the two access points. This feature is only available through the Management Console.

### Management Console

1. Select Show RF Statistics from the Main Menu.
2. Select Link Test-[F4] to view the Connection Quality Test screen.
3. Enter the MAC address of the access point or device you want to communicate with. Press Enter
4. Press ESC to stop the test and return to the previous menu.

Copyright © 2002 Intel Corporation. Legal Information