# Windows Me, 98, and 95 Installation

## Plug and Play Installation

Most CardBus-enabled computers support plug and play installation of the PRO/100 S and SR Mobile Adapters under Windows Me, Windows 98, and Windows 95 OSR2. However, early versions of Windows 95 (950 or 950a) are not supported.

## LAN Drivers Available

The following drivers for Windows Me, Windows 98, and Windows 95 OSR2 are supplied with the PRO/100 S and SR Mobile Adapters:

- NDIS4 driver (E100BNT.SYS)

- NDIS5 driver (E100BNT5.SYS)

The best NDIS driver for your operating system will be installed by default using the following procedures:

- Windows Me
- Windows 98 Second Edition (SE)
- Windows 95 OSR2

## Windows Me

| NOTE: If your laptop computer does not have a CD-ROM drive, go to Making Floppy Disks.

You can install drivers for Intel adapters using either the Found New Hardware Wizard or the Intel® PRO Intelligent Installer.

- If you use the Intel PRO Intelligent Installer, installation is a one-step process. You can install drivers and Intel PROSet II at the same time.

- If you use the Found New Hardware Wizard to install drivers, you must first install the drivers and then use the Intel CD to install other adapter components such as Intel PROSet II.

#### Installation with the Intel® PRO Intelligent Installer

The Intel PRO Intelligent Installer enables you to install adapter drivers, configuration utilities, and other add-on components for Intel adapters. The Installer supports Windows* 98, 2000, XP, and NT* 4.0. For Windows 95, see the Win95 folder on the CD-ROM shipped with your Intel® PRO/100 adapter.

For directions on installing drivers using the Installer, see Run the Installer.

#### Installation with the Found New Hardware Wizard

To install drivers in Windows Me, use the following procedure:

1. Put the cover back on the computer and turn on the power.

2. Windows Me starts and detects the adapter. The "Add New Hardware" wizard starts. Click Next to continue.

3. Select the Removable Media CD-ROM option and put the Intel CD in your computer. If the Autorun screen appears, close it. Click Next to continue.

4. Windows Me searches for drivers and asks which driver to install. Choose "The Updated Driver," and click Next.

5. Windows copies the driver files to the computer.

6. Click Finish and restart your computer when prompted.

7. Install Intel PROSet to configure and test the adapter. See Run the Installer (if you have a modem, use the Custom setting as described in the next step).

8. For your PRO/100 Combo Mobile Adapter, be sure the Drivers component, the Intel® PROSet II Wired Component, and the Intel® PRO/100 Mobile Modem Utilities Configuration Tool component are all configured for installation on the local drive. (After installation, the modem utilities will be accessible using Start > Programs > Intel(R) PRO-100 Mobile Modem Utilities.)

9. For most networks, you will need to configure properties for your protocols, computer identification, and preferred servers. Contact your network administrator for details if you need assistance.

10. Use your communications software to configure and operate the modem. For instruction on how to use modem AT commands, see Modem Information.

### Installation Notes for Windows Me

If you will be installing Windows Me or if you will be upgrading the adapter drivers in a multi-adapter Windows Me system, please read the following.

1. During installation of Windows Me (NOT during a driver installation on an existing Me computer), Windows Me may attempt to install its own older drivers on your new adapter and will appear successful. However upon reboot, you will find the adapter does not work. (It will install older adapters, but will not install your new adapter correctly.) If you check in Device Manager you will see that the adapter appears under Other Devices instead of under Network Devices. To make the adapter work, you must update the adapter driver with those included on the Intel CD.
   To update the driver go to Device Manager, select the adapter, and click Properties. Select the Driver tab and click the Update Driver button. Using the Update driver wizard, be very careful to choose the 'Search for a better driver... Removable Media (floppy, CD-ROM)' option and be sure Windows points to the drive of your inserted media. For a more detailed update procedure, visit http://support.intel.com

2. If you have multiple Intel adapters in your Windows Me system, you must be sure to update all of the Intel adapters to the software included with your new card. (See item 1 for driver update procedures. Repeat for each adapter). Failing to update any other Intel adapter in the system will cause the new adapter not to function. The failure will look as though the new adapter did not receive the proper update when you loaded the new driver, but this is NOT the case.
   The problem is that Windows Me cannot find the new driver while an older driver still exists on another adapter, so all other Intel adapters must be updated to the new driver. While updating, be very careful to choose the Removable Media (floppy/CD-ROM) option and be sure Windows points to the drive of your inserted media. Do not attempt to use any drivers already in any system directory.

## Windows 98 Second Edition (SE)

| NOTE: If your laptop computer does not have a CD-ROM drive, go to Making Floppy Disks.

#### Installation with the Intel® PRO Intelligent Installer

The Intel PRO Intelligent Installer enables you to install adapter drivers, configuration utilities, and other add-on components for Intel adapters. The Installer supports Windows* 98, 2000, XP, and NT* 4.0. For Windows 95, see the Win95 folder on the CD-ROM shipped with your Intel® PRO/100 adapter.

For directions on installing drivers using the Installer, see Run the Installer.

#### Installation with the Found New Hardware Wizard

1. After you put the adapter in the server and connect the cable, start Windows 98. You’ll see the New Hardware Found dialog box.

2. When prompted, insert the Intel CD.

3. For the path, type D:\ (for a CD-ROM drive) and then click OK.

4. Restart the system when prompted.

5. Install Intel PROSet to configure and test the adapter. See Run the Installer (if you have a modem, use the Custom setting as described in the next step).

6. For your PRO/100 Combo Mobile Adapter, be sure the Drivers component, the Intel® PROSet II Wired Component, and the Intel® PRO/100 Mobile Modem Utilities Configuration Tool component are all configured for installation on the local drive. (After installation, the modem utilities will be accessible using Start > Programs > Intel(R) PRO-100 Mobile Modem Utilities.)

7. For most networks, you will need to configure properties for your protocols, computer identification, and preferred servers. Contact your network administrator for details if you need assistance.

8. Use your communications software to configure and operate the modem. For instruction on how to use modem AT commands, see Modem Information.

### Updating the Network Drivers in Windows 98

You can update drivers using either the Update Device Driver wizard or the Intel CD.

#### Updating with the Intel CD

You can update drivers using the autorun program on the Intel CD.

1. Insert the Intel CD in the CD-ROM drive.
   The CD autorun program starts.

2. Click Update Drivers.

Intel adapter drivers automatically update.

#### Updating with the Update Device Driver Wizard

1. From the Control Panel, double-click the System icon.

2. Click the Device Manager tab.

3. Double-click Network Adapters in the list area.

4. Double-click the Intel® adapter.

5. Click on the Driver tab.

6. Click on the Update Driver button.

7. Click on the Next button.

8. Click on the circle next to the "Display a list of the drivers in a specific location..." (Do not select "Choose the updated driver...").

9. Click on the Have Disk button.

10. Insert the Networking Drivers Media in to the computer.

11. Type the drive letter of the Networking Drivers Media drive into the option box below "Copy manufacturer's files from:".

12. Click on the OK button.

13. Highlight the Intel® adapter, then click the OK button.

14. Click on the Next button in the Update Device Driver Wizard.

15. Insert the Windows 98 Disk when prompted, click OK.

16. Click the Finish button.

17. Restart the computer.

18. After restarting the computer, install Intel PROSet to configure and test the adapter. See Run the Intelligent Installer.

For troubleshooting information, go to Diagnostics and Troubleshooting.

## Windows 95 OSR2

| NOTE: If your laptop computer does not have a CD-ROM drive, go to Making Floppy Disks.

To install drivers in Windows 95, use the following procedure:

1. Power on the computer and allow Windows 95 to complete startup.

2. Insert the PRO/100 S or SR Mobile Adapter into the CardBus slot and connect cables as shown in Hardware Installation.

3. Windows detects a PCI Ethernet controller and displays the Update Device Driver Wizard. In this procedure, the LAN driver will be installed first and then the modem driver. Insert the Intel CD and click Next to start the procedure. (If the New Hardware Found window does NOT appear, you may need to enable CardBus support in your computer BIOS. See your computer's manual for information or check their website.)

4. Windows confirms the device name. Click Finish. This installs the LAN driver. If prompted for the NET82557.INF file, change the path back to your Intel CD. Windows may also ask you for the location of Windows networking files. Usually these are located in C:\windows\options\cabs or on your Windows 95 installation CD.

5. If prompted to restart, click Yes if you have the PRO/100 S or SR LAN only adapter and proceed to step 7.
   Click No if you have the PRO/100 S or SR Combo adapter and proceed to step 6.

6. Windows detects the modem portion of the adapter (PCI Serial Controller) and repeats the process above for the modem component. If prompted for other files, try changing the path to the Intel CD.

| NOTE: Windows may display a message indicating some VXD files are out of date. To determine if this affects operation of your computer, restart and check the modem. If it will not function, see the Mobile Release Notes file for detailed information.

7. Restart the computer for the configuration to take effect.

8. If you are not in the U.S. or Canada, run the Country Identifier utility to specify your location. The utility is located in the Intel Mobile program group.

For most networks, you will need to configure properties for your protocols, computer identification, and preferred servers. Contact your network administrator for details if you need assistance.

Have your Windows 95 installation CD or diskettes available; you’ll be prompted for them when you install the new adapter.

1. After you put the adapter in the computer and connect the cable, start the computer. Windows detects the adapter as a PCI Ethernet device.

2. Depending on your version of Windows 95, you'll see either the "Update Device Driver Wizard" or "New Hardware Found" window.

3. In either case, insert the Intel CD in your drive and wait for it to spin up. You may see an Introductory autorun screen open up after inserting the CD. Close this window if it appears.

4. Follow the instructions in the Windows prompts. When prompted for a path, type D:\ (for a CD-ROM drive) and then click OK.

5. Follow the prompts for any Windows 95 installation disks and restart the computer when prompted.

| NOTE: If you installed from the CD, the installation files are typically located at D:\Win95, where D is your CD-ROM drive.

After restarting Windows 95, connect to your network by double-clicking the Network Neighborhood icon on the desktop.

For troubleshooting information, go to Diagnostics and Troubleshooting.

## Installing and Using Intel PROSet II

For information about installing and using PROSet II to view link and activity status, to test hardware, and to set standard and advanced adapter features, see Installing with the Intel PRO Intelligent Installer.

## Modem Installation Troubleshooting

For information about troubleshooting when modem initialization errors or occur, when modem connection fails, or when other problems related to the modem occur, see Modem Installation Troubleshooting.

Copyright © 2002 Intel Corporation. Legal Information