## Known Access Points

The Intel® PRO/Wireless 2011B LAN Access Point can display a list of the known access points on the network derived from access point-to-access point communication. The list includes the MAC and IP addresses and configuration information for each access point. The first access point on the list provides the information. The access point recognizes other access points listed in subsequent lines. A broadcast message to access points every 12 seconds determines this list.

| NOTE: The Save All APs function from the Special Functions Menu updates and configures access point firmware and HTML code for all access points shown in the Known APs menu. You can perform this option only among the same hardware platforms and firmware versions.

### Web Interface

1. Select Known APs from the Statistics Menu at the left side of the screen.
2. Click Start Refresh to update the values on the screen.
3. When finished, click Stop Refresh.

### Management Console

1. Select Show Known APs from the Main Menu .
2. View more screens by selecting Next-[F3] Previous-[F4] at the bottom of the display.
3. You can view items by MAC Address or IP Address by selecting Switch at the bottom of the display.
4. Press ESC to return to the previous menu

### Parameter Descriptions

MAC Address | the unique 48-bit, hard-coded Media Access Control address, also known as the devices station identifier
IP Address | the network-assigned Internet Protocol address
DS Channel | The direct-sequence channel used by the access point.
computerS | The clients associated with the access point.
KBIOS | The data traffic handled by the access point in kilobytes in and out per second
FW_Ver | the firmware version used by the specified access point
Away | Determines if the access point functions as a part of the network or away . Away indicates the last known transmission took place 12 or more seconds before.

Copyright © 2002 Intel Corporation. Legal Information